 ==================================================================================
 BIOS Version : 02.16.00                                  Release Date : 05/15/2024
 Filename : IER50_BIOS_021600.BIN                         Checksum : 80895f9f(CRC32) 
                                                                     6c597d53a31afa0f07bcff577226aa0b(MD5) 
                                                                     f80c4a444f2dd9873e35604303a1af6bf4f3bd88(SHA1) 
 Filename : IER50_BIOS_021600.cpm                         Checksum : ac71a26b(CRC32) 
                                                                     6ce271028faf826e7c35202ece24bb11(MD5) 
                                                                     0a7f422c3900d4ded497d6ac275944d530741643(SHA1) 
 RC Revision : 109.D34                                    SPS Version : SPS_E5_06.01.04.047.0                        
 Microcode Version : m_10_806f8_2c000390.pdb
                     m_87_806f8_2b0005c0.pdb
                     m_87_c06f2_21000230.pdb
 Source Code : 5.32_EagleStreamCrb_0ACOR_102
 Flash Tools Path : http://epbua26fwsystem\attachments\download\15813\AFU_5.15.03.0081.7z
 ================================================================================== 
 1.Add function info into WEB Pcie Devices inventory page.
 2.Follow BMC spec, add new command for "Set NCSI Present".
 3.Add IPMI command of POST-Midway between POST-start and POST-end to notice BMC.
 4.Update Memory Controller information(ID & Name) in WEB inventory.
 5.The information of FirmwareVersion is empty in WEB Storage inventory page.
 6.Map ACPI_OEM_REV to BIOS version.
 7.Report PCH M2 slot by using ACPI method(_SUN).
 8.Update CRB to 5.32_EagleStreamCrb_0ACOR_102.
 9.Read MSR 0x1AD[7:0] to get MaxRatio as CPU Max speed.
 10.Show "Enable LP [Global]"(Hyper Threading) inside BIOS setup.
 11.Publish item "Enable LP [Global]"(Hyper Threading) for REDFISH.
 12.Defect #15820: [720][FERA1][Standard]SUT can't power on after swap DC-SCM board.
 13.Hide BmcSupport and IPMI InterfaceType option.
 14.Give actual boot device name for each BootXXXX in REDFISH.
 15.Show "SNC" item for all Customers.

 ==================================================================================
 BIOS Version : 02.15.00                                  Release Date : 01/15/2024
 Filename : IER50_BIOS_021500.BIN                         Checksum : 89b02a8c(CRC32) 
                                                                     29592db015c90bafc702c9bfe8529709(MD5) 
                                                                     b467c1b7f6b3858d4029b51b165fa83d0f55ec7e(SHA1) 
 Filename : IER50_BIOS_021500.cpm                         Checksum : 8509e4eb(CRC32) 
                                                                     919090861ab015e816e1fb2ee2d597ae(MD5) 
                                                                     646ed1e2fc8d88292a2040ce7217a2b3a07a83ba(SHA1) 
 RC Revision : 107.D52                                    SPS Version : SPS_E5_06.01.04.005.0                         
 Microcode Version : m_10_806f8_2c000351.pdb
                     m_87_806f8_2b000571.pdb
                     m_87_c06f2_21000200.pdb
 Source Code : 5.32_EagleStreamCrb_0ACOR_100
 Flash Tools Path : http://epbua26fwsystem\attachments\download\15813\AFU_5.15.03.0081.7z
 ================================================================================== 
 Update the BKC to 2023_WW49 to support SPR and EMR CPUs concurrently.
 
 ==================================================================================
 BIOS Version : 02.14.00                                  Release Date : 12/27/2023
 Filename : IER50_BIOS_021400.BIN                         Checksum : bc2f1b3d(CRC32) 
                                                                     8b5c74d806359e3090aefe51fc492b93(MD5) 
                                                                     7b3a69b5a71d3972c2152ac805bca81c1a545cc7(SHA1) 
 RC Revision : 100.D45                                    SPS Version : SPS_E5_06.00.04.070.0                        
 Microcode Version : m_10_806f8_2c0001d1.pdb
                     m_87_806f8_2b000461.pdb
                     m_87_c06f1_20000270.pdb
 Source Code : 5.31_EagleStreamCrb_0ACOR_080
 Flash Tools Path : http://epbua26fwsystem\attachments\download\15813\AFU_5.15.03.0081.7z
 ================================================================================== 
 1. Add the communication command to BMC to check if the RAID card exists in system.
 2. Remove "System Event Log" option of bios setup menu.
 
 ==================================================================================
 BIOS Version : 02.13.00                                  Release Date : 09/22/2023
 Filename : IER50_BIOS_021300.BIN                         Checksum : c05c6fc2(CRC32) 
                                                                     40f3f4030d893f940a0bdb598adbb7f0(MD5) 
                                                                     a03d035cf31614751814a09a8e32e4573ae6e1d8(SHA1) 
 RC Revision : 100.D45                                    SPS Version : SPS_E5_06.00.04.070.0                        
 Microcode Version : m_10_806f8_2c0001d1.pdb
                     m_87_806f8_2b000461.pdb
                     m_87_c06f1_20000270.pdb
 Source Code : 5.31_EagleStreamCrb_0ACOR_080
 Flash Tools Path : http://epbua26fwsystem\attachments\download\15813\AFU_5.15.03.0081.7z
 ================================================================================== 
 Set performance mode to Balanced mode as default.
 
 ==================================================================================
 BIOS Version : 02.12.00                                  Release Date : 09/21/2023
 Filename : IER50_BIOS_021200.BIN                         Checksum : 8437b639(CRC32) 
                                                                     70f7edb70f8e7f726ecffa8b6ad0f877(MD5) 
                                                                     1658252e7bb6a6edcfbac1d6048b92d6b245136f(SHA1) 
 RC Revision : 100.D45                                    SPS Version : SPS_E5_06.00.04.070.0                        
 Microcode Version : m_10_806f8_2c0001d1.pdb
                     m_87_806f8_2b000461.pdb
                     m_87_c06f1_20000270.pdb
 Source Code : 5.31_EagleStreamCrb_0ACOR_080
 Flash Tools Path : http://epbua26fwsystem\attachments\download\15813\AFU_5.15.03.0081.7z
 ==================================================================================
 Change Request #14003:[440] Suggest to add the share NIC LAN channel information under POST and BIOS setup menu.
 Show the BMC Share NIC IP(LAN Channel 3) info in BIOS setup menu.

 ==================================================================================
 BIOS Version : 02.11.00                                  Release Date : 09/13/2023
 Filename : IER50_BIOS_021100.BIN                         Checksum : cae99c3d(CRC32) 
                                                                     3ebf41f55da13658277dae8a05046ebc(MD5) 
                                                                     dc0bdd8aedc73355fca78d452fd9e14e2bf39cb2(SHA1) 
 RC Revision : 100.D45                                    SPS Version : SPS_E5_06.00.04.070.0                        
 Microcode Version : m_10_806f8_2c0001d1.pdb
                     m_87_806f8_2b000461.pdb
                     m_87_c06f1_20000270.pdb
 Source Code : 5.31_EagleStreamCrb_0ACOR_080
 Flash Tools Path : http://epbua26fwsystem\attachments\download\15813\AFU_5.15.03.0081.7z
 ================================================================================== 
 1.Show the BMC Share NIC IP(LAN Channel 3) info in early video of BIOS POST stage. 
 
 ==================================================================================
 BIOS Version : 02.10.00                                  Release Date : 08/30/2023
 Filename : IER50_BIOS_021000.BIN                         Checksum : 0b5a1408(CRC32) 
                                                                     bbe9b1b4ed23047fa7228213218ba3dd(MD5) 
                                                                     3f65460a8a4c904c104d424218f3edcafa02b0a3(SHA1) 
 RC Revision : 100.D45                                    SPS Version : SPS_E5_06.00.04.070.0                        
 Microcode Version : m_10_806f8_2c0001d1.pdb
                     m_87_806f8_2b000461.pdb
                     m_87_c06f1_20000270.pdb
 Source Code : 5.31_EagleStreamCrb_0ACOR_080
 Flash Tools Path : http://epbua26fwsystem\attachments\download\15813\AFU_5.15.03.0081.7z
 ================================================================================== 
 Add the JP18/JP19 auto bifurcation function for PVT MB.
 
 Note:
 When JP18 no cable connected, JP19 is x4x4(Socket 1: Port 5A,5C).
 When JP18 cable connected, JP18 + JP19 is x16 (Socket 1: Port 5A) for riser card upper slot.

 ==================================================================================
 BIOS Version : 01.09.00                                  Release Date : 08/22/2023
 Filename : IER50_BIOS_010900.BIN                         Checksum : fb5b2ce0(CRC32) 
                                                                     1ff9132d22ebbc69250deb434c2a204b(MD5) 
                                                                     70418cdd8b480695234488089df2a1d95412370b(SHA1) 
 RC Revision : 100.D45                                    SPS Version : SPS_E5_06.00.04.070.0                         
 Microcode Version : m_10_806f8_2c0001d1.pdb
                     m_87_806f8_2b000461.pdb
                     m_87_c06f1_20000270.pdb
 Source Code : 5.31_EagleStreamCrb_0ACOR_080
 Flash Tools Path : http://epbua26fwsystem\attachments\download\15813\AFU_5.15.03.0081.7z
 ================================================================================== 
 1.Change Request #14399:[440] Recommend to display the "Rank Sparing" option under BIOS Setup menu.
 2.Defect #14134:[640] System will randomly hang at POST 0x92 during OS reboot and AC cycle.
 
  ==================================================================================
 BIOS Version : 01.08.00                                  Release Date : 07/12/2023
 Filename : IER50_BIOS_010800.BIN                         Checksum : 07658d7b(CRC32) 
                                                                     f444c2826a83f25e9860cd62da5a07a7(MD5) 
                                                                     dc19e41f25ca4677c14062b085ff671c83137bc4(SHA1) 
 RC Revision : 100.D45                                    SPS Version : SPS_E5_06.00.04.070.0                        
 Microcode Version : m_10_806f8_2c0001d1.pdb
                     m_87_806f8_2b000461.pdb
                     m_87_c06f1_20000270.pdb
 Source Code : 5.31_EagleStreamCrb_0ACOR_080
 Flash Tools Path : http://epbua26fwsystem\attachments\download\15813\AFU_5.15.03.0081.7z
 ================================================================================== 
 1.Defect #14229:[440] SMBIOS Type 8 does not match the USB silkscreen on the TOP IO board.
 2.Defect #14266:[600] Node hangs in early video after changing the setting from "Mirror Mode" to "Full Mirror Mode".
 3.Defect #14207:[440] 9560-8i RAID card bandwidth will be downgraded after manual AC/DC/Reboot.
   Set item "PCI-E ASPM Support(Global)" to Disabled

 ==================================================================================
 BIOS Version : 01.07.00                                  Release Date : 07/03/2023
 Filename : IER50_BIOS_010700.BIN                         Checksum : 3565c1db(CRC32) 
                                                                     7ade1e8889114417fa08a54eeb1b38f9(MD5) 
                                                                     a3d30b98d4e8365739e1e74088a6cf7f84160caf(SHA1) 
 RC Revision : 100.D45                                    SPS Version : SPS_E5_06.00.04.070.0                        
 Microcode Version : m_10_806f8_2c0001d1.pdb
                     m_87_806f8_2b000461.pdb
                     m_87_c06f1_20000270.pdb
 Source Code : 5.31_EagleStreamCrb_0ACOR_080
 Flash Tools Path : http://epbua26fwsystem\attachments\download\15813\AFU_5.15.03.0081.7z
 ================================================================================== 
 1.Defect #14228: [440] SMBIOS Type 8 does not match server board layout for system SPEC V.11
 2.Defect #14229: [440] SMBIOS Type 8 does not match the USB silkscreen on the TOP IO board.
 3.Defect #14238: [520] Sensor name show "unknown" under BMC sel log after triggering PCIE correctable error via PEI 5.0.
 4.Defect #14210: [480] Cpu & Memory information is randomly and unstably read in "System Inventory" under BMC web.
 5.Defect #14233: [600] The BMC IP and CMC board IP under the BIOS setup menu will suddenly disappear in the idle state.
 6.The MCTP bus owner value will be programmed automatically due to the P2P bridge Bus:Device:Function of AST2600 will change when M.2 NVME device installed.
 7.Follow BMC's request, Modify settings of SDR USB Connect Status Event, SDR Inlet Temperature, SDR Outlet Temperature.
 8.Hidden unused options for IOUx (IIO PCIe Port x).
 
 ==================================================================================
 BIOS Version : 01.06.00                                  Release Date : 05/23/2023
 Filename : IER50_BIOS_010600.BIN                         Checksum : 1aa8e7e1(CRC32)
                                                                     9932401b1d9fc826a96fad51cdc2c55d(MD5)
                                                                     e81d36f295e0bf38ad088d282248be36c3d6f7ec(SHA1)
 RC Revision : 100.D45                                    SPS Version : SPS_E5_06.00.04.070.0
 Microcode Version : m_10_806f8_2c0001d1.pdb
                     m_87_806f8_2b000461.pdb
                     m_87_c06f1_20000270.pdb
 Source Code : 5.31_EagleStreamCrb_0ACOR_080
 Flash Tools Path : http://epbua26fwsystem\attachments\download\15813\AFU_5.15.03.0081.7z
 ==================================================================================
 1.Defect #14079: [440] Option Socket2 and Socket3 Configuration will appear under "IIO Configuration" and "Intel VMD technology" after BIOS restore default.
 2.Follow BMC's request, set OEM Power Sensor & OEM Outlet Temperature from Disabled to 200ms.

 ==================================================================================
 BIOS Version : 00.05.00                                  Release Date : 05/02/2023
 Filename : IER50_BIOS_000500.BIN                         Checksum : c60d454f(CRC32)
                                                                     6701bd57dd32577c50fae3f27fdb19d3(MD5)
                                                                     1b6ae8a9b9ac6e48ad27162402aff2567521ffdb(SHA1)
 RC Revision : 100.D45                                    SPS Version : SPS_E5_06.00.04.070.0
 Microcode Version : m_10_806f8_2c0001d1.pdb
                     m_87_806f8_2b000461.pdb
                     m_87_c06f1_20000270.pdb
 Source Code : 5.31_EagleStreamCrb_0ACOR_080
 Flash Tools Path : http://epbua26fwsystem\attachments\download\15813\AFU_5.15.03.0081.7z
 ==================================================================================
 1.Defect #13935: [440] Sensor name and sensor type under BMC SEL doesn't match "Sensor of BIOS" in BMC SPEC after injecting PCIe error.
 2.Update BKC 2023_WW13.

 ==================================================================================
 BIOS Version : 00.04.00                                  Release Date : 03/31/2023
 Filename : IER50_BIOS_000400.BIN                         Checksum : a23e10d6(CRC32)
                                                                     559957847edbd0edc582496db53d32fd(MD5)
                                                                     0c73c8c722069631e170ae12400899bb34a84d9a(SHA1)
 RC Revision : 9409.P09                                    SPS Version : SPS_E5_06.00.04.025.0
 Microcode Version : m_10_806f8_2c000170.pdb
                     m_87_806f8_2b000181.pdb
 Source Code : 5.29_EagleStreamCrb_0ACOR_073
 Flash Tools Path : http://epbua26fwsystem\attachments\download\15813\AFU_5.15.03.0081.7z
 ==================================================================================
 1.Defect #13913: [440] Device Locator String of SMBIOS type 17 does not match with System SPEC V08
 2.Defect #13910: [440] Memory Topology Information under BIOS setup does not match with the DIMM silkscreen on MB
 3.Change the USB OC OEMEvData1 from 00h to F4h follow BMC spec.

 ==================================================================================
 BIOS Version : 00.03.00                                  Release Date : 03/16/2023
 Filename : IER50_BIOS_000300.BIN                         Checksum : a7a26198(CRC32)
                                                                     5cc9f7b51309cf198f7e23e79927580d(MD5)
                                                                     f3a9ed01570b422f812a9b18568a509dc6d34df3(SHA1)
 RC Revision : 9409.P09                                   SPS Version : SPS_E5_06.00.04.025.0
 Microcode Version : m_10_806f8_2c000170.pdb
                     m_87_806f8_2b000181.pdb
 Source Code : 5.29_EagleStreamCrb_0ACOR_073
 Flash Tools Path : http://epbua26fwsystem\attachments\download\15813\AFU_5.15.03.0081.7z
 ==================================================================================
 1.Change eSPI mode to Single mode(same as CRB).
 2.Adjust the SATA parameters on all SATA ports(HsioTxGen3DeEmphEnable = TRUE, HsioTxGen3DeEmph = 0x28).
 3.Add the HDD numbering(0~3) string concatenate the SATA Controller 2(1-Base) Port(4~7).
 4.Set 0 to related field for improving USB chip to chip signal.

 ==================================================================================
 BIOS Version : 00.02.00                                  Release Date : 02/18/2023
 Filename : IER50_BIOS_000200.BIN                         Checksum : aa50b3a0(CRC32)
                                                                     51605ed1996333c543bd0d46808a1bef(MD5)
                                                                     f3536bc9dae78781a2c0657e0c4ef77a0b46d53b(SHA1)
 RC Revision : 9409.P09                                    SPS Version : SPS_E5_06.00.04.025.0
 Microcode Version : m_10_806f8_2c000170.pdb
                     m_87_806f8_2b000181.pdb
 Source Code : 5.29_EagleStreamCrb_0ACOR_073
 Flash Tools Path : http://epbua26fwsystem\attachments\download\15813\AFU_5.15.03.0081.7z
 ==================================================================================
 1. Update the sign key to enable the BMC web BIOS firmware update feature.
 2. Enable the BIOS PFR feature.

 ==================================================================================
 BIOS Version : 00.01.00                                  Release Date : 02/09/2023
 Filename : IER50_BIOS_000100.BIN                         Checksum : bf9683ec(CRC32)
                                                                     04d33aa069b21ce123e1cf95d081cd79(MD5)
                                                                     0a2812ac8140cb67e874355c0509cc7b0674d264(SHA1)
 RC Revision : 9409.P09                                    SPS Version : SPS_E5_06.00.04.025.0
 Microcode Version : m_10_806f8_2c000170.pdb
                     m_87_806f8_2b000181.pdb
 Source Code : 5.29_EagleStreamCrb_0ACOR_073
 Flash Tools Path : http://epbua26fwsystem\attachments\download\15813\AFU_5.15.03.0081.7z
 ==================================================================================
 1. First release