Folder format:

    - ROM/       : Update ROM/Binary by offline IC programmer.

    - WebUpdate/ : Update ROM/Binary by BMC web.


For manufacture notice of Winbond IC Flash:
    - When offline update ROM/Binary on Winbond Flash chip and boot fail, please follow the PDF file which setup driver strength by IC programmer.

    - Example of PDF file: "Use HI-LO ALL-200G to setup driver strength on Winbond NOR Flash.pdf"

