*************************************************************************************
* Version:       10.06.00
* System:        JER25 
*   
* Release Date:  2/27/2025
* File Name:     JER25_BIOS_100600.bin 
*
* CRC32 CheckSum: BDD264A1
* SHA1  CheckSum: 8f75f5bef7485b3433d026c936d5847765d833ca
* MD5   CheckSum: c8da0707c4d7ec4a7a4a5218d1b6177c
**************************************************************************************
Integrated module collateral:
 AMI CodeBase:
   Turin:0ACST_PI1.0.0.3_017 (PI 1.0.0.3 / PSP 00.3D.00.6C  / SMU 00.5E.73.00/ U Code (A0 0x0B00004D/B0 0x0B001016/C0 0x0B002032 /C1 0x0B00211E/Dense A0 0x0B10000F/Dense B0 0x0B101028)

---------------
Important Note:
---------------
  1.According AMD Doc#58401 Week-5, Update on 64MB SPI chip usage , It limited the BIOS 
    image update method . Please refer BIOS update SOP when boot with Turin ES1/2 CPU.
  2.Installing Windows Server 2019, 2022, or Windows 10, Windows 11, fails with a blue screen of death (BSOD) error and 
    the message "MULTIPROCESSOR CONFIGURATION NOT SUPPORTED" when installing on the listed AMD-based ThinkSystem platforms 
    that have 64+ cores per CPU package. 
   Workaround:
    1. Reduce the CPU core count in UEFI setting System Information -> Processors -> Number of Enabled CPU Cores Per" to 64C before OS installation.
    2. Install Microsoft Windows Server.
    3. Download and apply the latest Windows Monthly Update from Microsoft's website:
    For Win2022:
       https://support.microsoft.com/en-us/topic/windows-server-2022-update-history-e1caa597-00c5-4ab9-9f3e-8212fe80b2ee
    For Win2019:
       https://support.microsoft.com/en-us/topic/windows-10-and-windows-server-2019-update-history-725fc2e1-4443-6831-a5ca-51ff5cbcb059.
  3. After the update installation is completed, reboot the system and re-enable all CPU cores. The OS should then function as expected.
  4. For Windows client OS (Windows 10 or Windows 11), the recommendation is to download and install 22H2 of Windows 11 to support this type of high core count CPUs.
  5. PCIe Root Bridge has exchange from PI 0.0.8.0 . Therefor the Bus number assign has change , (Before: G3=0x20 , P3=0x60 . After: G3=0x60 , P3=0x20)
  6.Enable PFR function , but request PC (C0 stepping) CPU to support it 
  7.Request BMC verison V0.11.0
  8.BIOS start support NMI funciotn , Need to use BMC V0.15.00 to avoid system hang .
  9.Enable Secure Flash for HSI spport for WS2022 Cert, and it will change BIOS image layout.
    Please does not use AMI AFU tool to upgrade/downgrade BIOS version from EVT/DVT/PVT to RTM BIOS (version: 10.01.00)
-------------
Known Issues:
-------------
  1.BIOS version & CPU stepping matrix trble.
  ---------------------------------------------------------------------------------------------------------------------------------------------------
  |CPU Stepping  |  BIOS Verison  |  Flash Size   |  Prgramming Setting    |  PFR Verify    |  Notice                     
  |                                                                                                                                                                          
  |                        | 1.3.0 & Before  |   32 MB        | Default Setting             |         No        |  N/A                         
  |     A0 / B0                                                                                                                                                           
  |                        | 1.3.0 & Before  |   64 MB        | programming address  |         No        |  N/A                          
  |                                                                         from 0x2000000            |                                                        
  |---------------------------------------------------------------------------------------------------------------------------------------------------
  |                        | 1.4.0 & later     |   32 MB      | Default Setting               |         No        |  N/A                          
  |     A0 / B0                                                                                                                                                        
  |                        | 1.4.0 & later     |   64 MB      | programming address    |         No        |  1.System will random hang during POST
  |                                                                     | from 0x2000000              |         No        |  2.BIOS setup menu value can't chamge  
  |----------------------------------------------------------------------------------------------------------------------------------------------------
  |                        | 1.3.0 & Before  |   32 MB        | Default Setting             |         No        |  System can't boot                    
  |     C0                                                                                                                                                           
  |                        | 1.3.0 & Before  |   64 MB        |  Default Setting            |         No        |   System can't boot                       
  | ------------------------------------------------------------------------------------------------------------------------------------------------------- 
  |                        | 1.4.0 & later     |   32 MB      | Default Setting             |         Yes       |  N/A                         
  |     C0                                                                                                                                                           
  |                        | 1.4.0 & later     |   64 MB      |  Default Setting            |        Yes        |  N/A                          
  | ------------------------------------------------------------------------------------------------------------------------------------------------------- 

------------
Changes:
------------
1. Upgrade PI code to 1.0.0.3.

*************************************************************************************
* Version:       10.05.00
* System:        JER25 
*   
* Release Date:  2/13/2025
* File Name:     JER25_BIOS_100500.bin 
*
* CRC32 CheckSum: C36320D2
* SHA1  CheckSum: 4cf99dbcc47613cfaaa320a4f29f6dda313ec8b5
* MD5   CheckSum: f8bb9c4704f8524cb5fcfa1c6eaaf721
**************************************************************************************
Integrated module collateral:
 AMI CodeBase:
   Turin:0ACST_PI1.0.0.1_015 (PI 1.0.0.1 / PSP 00.3D.00.65  / SMU 00.5E.6C.00/ U Code (A0 0x0B00004D/B0 0x0B001016/C0 0x0B00202B /C1 0x0B002116/Dense A0 0x0B10000F/Dense B0 0x0B101021)

---------------
Important Note:
---------------
  1.According AMD Doc#58401 Week-5, Update on 64MB SPI chip usage , It limited the BIOS 
    image update method . Please refer BIOS update SOP when boot with Turin ES1/2 CPU.
  2.Installing Windows Server 2019, 2022, or Windows 10, Windows 11, fails with a blue screen of death (BSOD) error and 
    the message "MULTIPROCESSOR CONFIGURATION NOT SUPPORTED" when installing on the listed AMD-based ThinkSystem platforms 
    that have 64+ cores per CPU package. 
   Workaround:
    1. Reduce the CPU core count in UEFI setting System Information -> Processors -> Number of Enabled CPU Cores Per" to 64C before OS installation.
    2. Install Microsoft Windows Server.
    3. Download and apply the latest Windows Monthly Update from Microsoft's website:
    For Win2022:
       https://support.microsoft.com/en-us/topic/windows-server-2022-update-history-e1caa597-00c5-4ab9-9f3e-8212fe80b2ee
    For Win2019:
       https://support.microsoft.com/en-us/topic/windows-10-and-windows-server-2019-update-history-725fc2e1-4443-6831-a5ca-51ff5cbcb059.
  3. After the update installation is completed, reboot the system and re-enable all CPU cores. The OS should then function as expected.
  4. For Windows client OS (Windows 10 or Windows 11), the recommendation is to download and install 22H2 of Windows 11 to support this type of high core count CPUs.
  5. PCIe Root Bridge has exchange from PI 0.0.8.0 . Therefor the Bus number assign has change , (Before: G3=0x20 , P3=0x60 . After: G3=0x60 , P3=0x20)
  6.Enable PFR function , but request PC (C0 stepping) CPU to support it 
  7.Request BMC verison V0.11.0
  8.BIOS start support NMI funciotn , Need to use BMC V0.15.00 to avoid system hang .
  9.Enable Secure Flash for HSI spport for WS2022 Cert, and it will change BIOS image layout.
    Please does not use AMI AFU tool to upgrade/downgrade BIOS version from EVT/DVT/PVT to RTM BIOS (version: 10.01.00)
-------------
Known Issues:
-------------
  1.BIOS version & CPU stepping matrix trble.
  ---------------------------------------------------------------------------------------------------------------------------------------------------
  |CPU Stepping  |  BIOS Verison  |  Flash Size   |  Prgramming Setting    |  PFR Verify    |  Notice                     
  |                                                                                                                                                                          
  |                        | 1.3.0 & Before  |   32 MB        | Default Setting             |         No        |  N/A                         
  |     A0 / B0                                                                                                                                                           
  |                        | 1.3.0 & Before  |   64 MB        | programming address  |         No        |  N/A                          
  |                                                                         from 0x2000000            |                                                        
  |---------------------------------------------------------------------------------------------------------------------------------------------------
  |                        | 1.4.0 & later     |   32 MB      | Default Setting               |         No        |  N/A                          
  |     A0 / B0                                                                                                                                                        
  |                        | 1.4.0 & later     |   64 MB      | programming address    |         No        |  1.System will random hang during POST
  |                                                                     | from 0x2000000              |         No        |  2.BIOS setup menu value can't chamge  
  |----------------------------------------------------------------------------------------------------------------------------------------------------
  |                        | 1.3.0 & Before  |   32 MB        | Default Setting             |         No        |  System can't boot                    
  |     C0                                                                                                                                                           
  |                        | 1.3.0 & Before  |   64 MB        |  Default Setting            |         No        |   System can't boot                       
  | ------------------------------------------------------------------------------------------------------------------------------------------------------- 
  |                        | 1.4.0 & later     |   32 MB      | Default Setting             |         Yes       |  N/A                         
  |     C0                                                                                                                                                           
  |                        | 1.4.0 & later     |   64 MB      |  Default Setting            |        Yes        |  N/A                          
  | ------------------------------------------------------------------------------------------------------------------------------------------------------- 

------------
Changes:
------------
1. Rollback OEM PK certificate for WS2025 HSTI test.

*************************************************************************************
* Version:       10.04.00
* System:        JER25 
*   
* Release Date:  2/5/2025
* File Name:     JER25_BIOS_100400.bin 
*
* CRC32 CheckSum: 1CCDB856
* SHA1  CheckSum: 0de9810733526628d762cd23e56c8c3a4ef0b1be
* MD5   CheckSum: 40b90a5f3d45ca9315889a1c9e49efc7
**************************************************************************************
Integrated module collateral:
 AMI CodeBase:
   Turin:0ACST_PI1.0.0.1_015 (PI 1.0.0.1 / PSP 00.3D.00.65  / SMU 00.5E.6C.00/ U Code (A0 0x0B00004D/B0 0x0B001016/C0 0x0B00202B /C1 0x0B002116/Dense A0 0x0B10000F/Dense B0 0x0B101021)

---------------
Important Note:
---------------
  1.According AMD Doc#58401 Week-5, Update on 64MB SPI chip usage , It limited the BIOS 
    image update method . Please refer BIOS update SOP when boot with Turin ES1/2 CPU.
  2.Installing Windows Server 2019, 2022, or Windows 10, Windows 11, fails with a blue screen of death (BSOD) error and 
    the message "MULTIPROCESSOR CONFIGURATION NOT SUPPORTED" when installing on the listed AMD-based ThinkSystem platforms 
    that have 64+ cores per CPU package. 
   Workaround:
    1. Reduce the CPU core count in UEFI setting System Information -> Processors -> Number of Enabled CPU Cores Per" to 64C before OS installation.
    2. Install Microsoft Windows Server.
    3. Download and apply the latest Windows Monthly Update from Microsoft's website:
    For Win2022:
       https://support.microsoft.com/en-us/topic/windows-server-2022-update-history-e1caa597-00c5-4ab9-9f3e-8212fe80b2ee
    For Win2019:
       https://support.microsoft.com/en-us/topic/windows-10-and-windows-server-2019-update-history-725fc2e1-4443-6831-a5ca-51ff5cbcb059.
  3. After the update installation is completed, reboot the system and re-enable all CPU cores. The OS should then function as expected.
  4. For Windows client OS (Windows 10 or Windows 11), the recommendation is to download and install 22H2 of Windows 11 to support this type of high core count CPUs.
  5. PCIe Root Bridge has exchange from PI 0.0.8.0 . Therefor the Bus number assign has change , (Before: G3=0x20 , P3=0x60 . After: G3=0x60 , P3=0x20)
  6.Enable PFR function , but request PC (C0 stepping) CPU to support it 
  7.Request BMC verison V0.11.0
  8.BIOS start support NMI funciotn , Need to use BMC V0.15.00 to avoid system hang .
  9.Enable Secure Flash for HSI spport for WS2022 Cert, and it will change BIOS image layout.
    Please does not use AMI AFU tool to upgrade/downgrade BIOS version from EVT/DVT/PVT to RTM BIOS (version: 10.01.00)
-------------
Known Issues:
-------------
  1.BIOS version & CPU stepping matrix trble.
  ---------------------------------------------------------------------------------------------------------------------------------------------------
  |CPU Stepping  |  BIOS Verison  |  Flash Size   |  Prgramming Setting    |  PFR Verify    |  Notice                     
  |                                                                                                                                                                          
  |                        | 1.3.0 & Before  |   32 MB        | Default Setting             |         No        |  N/A                         
  |     A0 / B0                                                                                                                                                           
  |                        | 1.3.0 & Before  |   64 MB        | programming address  |         No        |  N/A                          
  |                                                                         from 0x2000000            |                                                        
  |---------------------------------------------------------------------------------------------------------------------------------------------------
  |                        | 1.4.0 & later     |   32 MB      | Default Setting               |         No        |  N/A                          
  |     A0 / B0                                                                                                                                                        
  |                        | 1.4.0 & later     |   64 MB      | programming address    |         No        |  1.System will random hang during POST
  |                                                                     | from 0x2000000              |         No        |  2.BIOS setup menu value can't chamge  
  |----------------------------------------------------------------------------------------------------------------------------------------------------
  |                        | 1.3.0 & Before  |   32 MB        | Default Setting             |         No        |  System can't boot                    
  |     C0                                                                                                                                                           
  |                        | 1.3.0 & Before  |   64 MB        |  Default Setting            |         No        |   System can't boot                       
  | ------------------------------------------------------------------------------------------------------------------------------------------------------- 
  |                        | 1.4.0 & later     |   32 MB      | Default Setting             |         Yes       |  N/A                         
  |     C0                                                                                                                                                           
  |                        | 1.4.0 & later     |   64 MB      |  Default Setting            |        Yes        |  N/A                          
  | ------------------------------------------------------------------------------------------------------------------------------------------------------- 

------------
Changes:
------------
1. Fix #17692. [OS Certification][WS2025] Assurance AQ fail at "NoPPIProvision is not set to false"
2. Fix #17691. [OS Certification][WS2025] Secure Boot Logo fail at "KEK” and “DB ”

*************************************************************************************
* Version:       10.03.00
* System:        JER25 
*   
* Release Date:  1/7/2025
* File Name:     JER25_BIOS_100300.bin 
*
* CRC32 CheckSum: BCBD57A0
* SHA1  CheckSum: 2a70012f96ac75aa4a693465502dcdf8dee1e2f2
* MD5   CheckSum: 1cc725e07fc965744f014b1b76ab44f5
**************************************************************************************
Integrated module collateral:
 AMI CodeBase:
   Turin:0ACST_PI1.0.0.1_015 (PI 1.0.0.1 / PSP 00.3D.00.65  / SMU 00.5E.6C.00/ U Code (A0 0x0B00004D/B0 0x0B001016/C0 0x0B00202B /C1 0x0B002116/Dense A0 0x0B10000F/Dense B0 0x0B101021)

---------------
Important Note:
---------------
  1.According AMD Doc#58401 Week-5, Update on 64MB SPI chip usage , It limited the BIOS 
    image update method . Please refer BIOS update SOP when boot with Turin ES1/2 CPU.
  2.Installing Windows Server 2019, 2022, or Windows 10, Windows 11, fails with a blue screen of death (BSOD) error and 
    the message "MULTIPROCESSOR CONFIGURATION NOT SUPPORTED" when installing on the listed AMD-based ThinkSystem platforms 
    that have 64+ cores per CPU package. 
   Workaround:
    1. Reduce the CPU core count in UEFI setting System Information -> Processors -> Number of Enabled CPU Cores Per" to 64C before OS installation.
    2. Install Microsoft Windows Server.
    3. Download and apply the latest Windows Monthly Update from Microsoft's website:
    For Win2022:
       https://support.microsoft.com/en-us/topic/windows-server-2022-update-history-e1caa597-00c5-4ab9-9f3e-8212fe80b2ee
    For Win2019:
       https://support.microsoft.com/en-us/topic/windows-10-and-windows-server-2019-update-history-725fc2e1-4443-6831-a5ca-51ff5cbcb059.
  3. After the update installation is completed, reboot the system and re-enable all CPU cores. The OS should then function as expected.
  4. For Windows client OS (Windows 10 or Windows 11), the recommendation is to download and install 22H2 of Windows 11 to support this type of high core count CPUs.
  5. PCIe Root Bridge has exchange from PI 0.0.8.0 . Therefor the Bus number assign has change , (Before: G3=0x20 , P3=0x60 . After: G3=0x60 , P3=0x20)
  6.Enable PFR function , but request PC (C0 stepping) CPU to support it 
  7.Request BMC verison V0.11.0
  8.BIOS start support NMI funciotn , Need to use BMC V0.15.00 to avoid system hang .
  9.Enable Secure Flash for HSI spport for WS2022 Cert, and it will change BIOS image layout.
    Please does not use AMI AFU tool to upgrade/downgrade BIOS version from EVT/DVT/PVT to RTM BIOS (version: 10.01.00)
-------------
Known Issues:
-------------
  1.BIOS version & CPU stepping matrix trble.
  ---------------------------------------------------------------------------------------------------------------------------------------------------
  |CPU Stepping  |  BIOS Verison  |  Flash Size   |  Prgramming Setting    |  PFR Verify    |  Notice                     
  |                                                                                                                                                                          
  |                        | 1.3.0 & Before  |   32 MB        | Default Setting             |         No        |  N/A                         
  |     A0 / B0                                                                                                                                                           
  |                        | 1.3.0 & Before  |   64 MB        | programming address  |         No        |  N/A                          
  |                                                                         from 0x2000000            |                                                        
  |---------------------------------------------------------------------------------------------------------------------------------------------------
  |                        | 1.4.0 & later     |   32 MB      | Default Setting               |         No        |  N/A                          
  |     A0 / B0                                                                                                                                                        
  |                        | 1.4.0 & later     |   64 MB      | programming address    |         No        |  1.System will random hang during POST
  |                                                                     | from 0x2000000              |         No        |  2.BIOS setup menu value can't chamge  
  |----------------------------------------------------------------------------------------------------------------------------------------------------
  |                        | 1.3.0 & Before  |   32 MB        | Default Setting             |         No        |  System can't boot                    
  |     C0                                                                                                                                                           
  |                        | 1.3.0 & Before  |   64 MB        |  Default Setting            |         No        |   System can't boot                       
  | ------------------------------------------------------------------------------------------------------------------------------------------------------- 
  |                        | 1.4.0 & later     |   32 MB      | Default Setting             |         Yes       |  N/A                         
  |     C0                                                                                                                                                           
  |                        | 1.4.0 & later     |   64 MB      |  Default Setting            |        Yes        |  N/A                          
  | ------------------------------------------------------------------------------------------------------------------------------------------------------- 

------------
Changes:
------------
1. Add MsSysGrd Module for cert test


*************************************************************************************
* Version:       10.02.00
* System:        JER25 
*   
* Release Date:  12/17/2024
* File Name:     JER25_BIOS_100200.bin 
*
* CRC32 CheckSum: B1B19DEC
* SHA1  CheckSum: 8d7626a3d2432d0b3a8233ee295b36a00b25e94b
* MD5   CheckSum: f67db0548def422dd8e6fe99071210cd
**************************************************************************************
Integrated module collateral:
 AMI CodeBase:
   Turin:0ACST_PI1.0.0.1_015 (PI 1.0.0.1 / PSP 00.3D.00.65  / SMU 00.5E.6C.00/ U Code (A0 0x0B00004D/B0 0x0B001016/C0 0x0B00202B /C1 0x0B002116/Dense A0 0x0B10000F/Dense B0 0x0B101021)

---------------
Important Note:
---------------
  1.According AMD Doc#58401 Week-5, Update on 64MB SPI chip usage , It limited the BIOS 
    image update method . Please refer BIOS update SOP when boot with Turin ES1/2 CPU.
  2.Installing Windows Server 2019, 2022, or Windows 10, Windows 11, fails with a blue screen of death (BSOD) error and 
    the message "MULTIPROCESSOR CONFIGURATION NOT SUPPORTED" when installing on the listed AMD-based ThinkSystem platforms 
    that have 64+ cores per CPU package. 
   Workaround:
    1. Reduce the CPU core count in UEFI setting System Information -> Processors -> Number of Enabled CPU Cores Per" to 64C before OS installation.
    2. Install Microsoft Windows Server.
    3. Download and apply the latest Windows Monthly Update from Microsoft's website:
    For Win2022:
       https://support.microsoft.com/en-us/topic/windows-server-2022-update-history-e1caa597-00c5-4ab9-9f3e-8212fe80b2ee
    For Win2019:
       https://support.microsoft.com/en-us/topic/windows-10-and-windows-server-2019-update-history-725fc2e1-4443-6831-a5ca-51ff5cbcb059.
  3. After the update installation is completed, reboot the system and re-enable all CPU cores. The OS should then function as expected.
  4. For Windows client OS (Windows 10 or Windows 11), the recommendation is to download and install 22H2 of Windows 11 to support this type of high core count CPUs.
  5. PCIe Root Bridge has exchange from PI 0.0.8.0 . Therefor the Bus number assign has change , (Before: G3=0x20 , P3=0x60 . After: G3=0x60 , P3=0x20)
  6.Enable PFR function , but request PC (C0 stepping) CPU to support it 
  7.Request BMC verison V0.11.0
  8.BIOS start support NMI funciotn , Need to use BMC V0.15.00 to avoid system hang .
  9.Enable Secure Flash for HSI spport for WS2022 Cert, and it will change BIOS image layout.
    Please does not use AMI AFU tool to upgrade/downgrade BIOS version from EVT/DVT/PVT to RTM BIOS (version: 10.01.00)
-------------
Known Issues:
-------------
  1.BIOS version & CPU stepping matrix trble.
  ---------------------------------------------------------------------------------------------------------------------------------------------------
  |CPU Stepping  |  BIOS Verison  |  Flash Size   |  Prgramming Setting    |  PFR Verify    |  Notice                     
  |                                                                                                                                                                          
  |                        | 1.3.0 & Before  |   32 MB        | Default Setting             |         No        |  N/A                         
  |     A0 / B0                                                                                                                                                           
  |                        | 1.3.0 & Before  |   64 MB        | programming address  |         No        |  N/A                          
  |                                                                         from 0x2000000            |                                                        
  |---------------------------------------------------------------------------------------------------------------------------------------------------
  |                        | 1.4.0 & later     |   32 MB      | Default Setting               |         No        |  N/A                          
  |     A0 / B0                                                                                                                                                        
  |                        | 1.4.0 & later     |   64 MB      | programming address    |         No        |  1.System will random hang during POST
  |                                                                     | from 0x2000000              |         No        |  2.BIOS setup menu value can't chamge  
  |----------------------------------------------------------------------------------------------------------------------------------------------------
  |                        | 1.3.0 & Before  |   32 MB        | Default Setting             |         No        |  System can't boot                    
  |     C0                                                                                                                                                           
  |                        | 1.3.0 & Before  |   64 MB        |  Default Setting            |         No        |   System can't boot                       
  | ------------------------------------------------------------------------------------------------------------------------------------------------------- 
  |                        | 1.4.0 & later     |   32 MB      | Default Setting             |         Yes       |  N/A                         
  |     C0                                                                                                                                                           
  |                        | 1.4.0 & later     |   64 MB      |  Default Setting            |        Yes        |  N/A                          
  | ------------------------------------------------------------------------------------------------------------------------------------------------------- 

------------
Changes:
------------
1. Un-Hide TSME knob for Windows Cert test requirement.


*************************************************************************************
* Version:       10.01.00
* System:        JER25 
*   
* Release Date:  12/10/2024
* File Name:     JER25_BIOS_100100.bin 
*
* CRC32 CheckSum: 26DD3BBA
* SHA1  CheckSum: f46fece2434e460b7122633f63dd0702c45028c8
* MD5   CheckSum: cb3264aa815a1cf2421530fe98e66dfa
**************************************************************************************
Integrated module collateral:
 AMI CodeBase:
   Turin:0ACST_PI1.0.0.1_015 (PI 1.0.0.1 / PSP 00.3D.00.65  / SMU 00.5E.6C.00/ U Code (A0 0x0B00004D/B0 0x0B001016/C0 0x0B00202B /C1 0x0B002116/Dense A0 0x0B10000F/Dense B0 0x0B101021)

---------------
Important Note:
---------------
  1.According AMD Doc#58401 Week-5, Update on 64MB SPI chip usage , It limited the BIOS 
    image update method . Please refer BIOS update SOP when boot with Turin ES1/2 CPU.
  2.Installing Windows Server 2019, 2022, or Windows 10, Windows 11, fails with a blue screen of death (BSOD) error and 
    the message "MULTIPROCESSOR CONFIGURATION NOT SUPPORTED" when installing on the listed AMD-based ThinkSystem platforms 
    that have 64+ cores per CPU package. 
   Workaround:
    1. Reduce the CPU core count in UEFI setting System Information -> Processors -> Number of Enabled CPU Cores Per" to 64C before OS installation.
    2. Install Microsoft Windows Server.
    3. Download and apply the latest Windows Monthly Update from Microsoft's website:
    For Win2022:
       https://support.microsoft.com/en-us/topic/windows-server-2022-update-history-e1caa597-00c5-4ab9-9f3e-8212fe80b2ee
    For Win2019:
       https://support.microsoft.com/en-us/topic/windows-10-and-windows-server-2019-update-history-725fc2e1-4443-6831-a5ca-51ff5cbcb059.
  3. After the update installation is completed, reboot the system and re-enable all CPU cores. The OS should then function as expected.
  4. For Windows client OS (Windows 10 or Windows 11), the recommendation is to download and install 22H2 of Windows 11 to support this type of high core count CPUs.
  5. PCIe Root Bridge has exchange from PI 0.0.8.0 . Therefor the Bus number assign has change , (Before: G3=0x20 , P3=0x60 . After: G3=0x60 , P3=0x20)
  6.Enable PFR function , but request PC (C0 stepping) CPU to support it 
  7.Request BMC verison V0.11.0
  8.BIOS start support NMI funciotn , Need to use BMC V0.15.00 to avoid system hang .
  9.Enable Secure Flash for HSI spport for WS2022 Cert, and it will change BIOS image layout.
    Please does not use AMI AFU tool to upgrade/downgrade BIOS version from EVT/DVT/PVT to RTM BIOS (version: 10.01.00)
-------------
Known Issues:
-------------
  1.BIOS version & CPU stepping matrix trble.
  ---------------------------------------------------------------------------------------------------------------------------------------------------
  |CPU Stepping  |  BIOS Verison  |  Flash Size   |  Prgramming Setting    |  PFR Verify    |  Notice                     
  |                                                                                                                                                                          
  |                        | 1.3.0 & Before  |   32 MB        | Default Setting             |         No        |  N/A                         
  |     A0 / B0                                                                                                                                                           
  |                        | 1.3.0 & Before  |   64 MB        | programming address  |         No        |  N/A                          
  |                                                                         from 0x2000000            |                                                        
  |---------------------------------------------------------------------------------------------------------------------------------------------------
  |                        | 1.4.0 & later     |   32 MB      | Default Setting               |         No        |  N/A                          
  |     A0 / B0                                                                                                                                                        
  |                        | 1.4.0 & later     |   64 MB      | programming address    |         No        |  1.System will random hang during POST
  |                                                                     | from 0x2000000              |         No        |  2.BIOS setup menu value can't chamge  
  |----------------------------------------------------------------------------------------------------------------------------------------------------
  |                        | 1.3.0 & Before  |   32 MB        | Default Setting             |         No        |  System can't boot                    
  |     C0                                                                                                                                                           
  |                        | 1.3.0 & Before  |   64 MB        |  Default Setting            |         No        |   System can't boot                       
  | ------------------------------------------------------------------------------------------------------------------------------------------------------- 
  |                        | 1.4.0 & later     |   32 MB      | Default Setting             |         Yes       |  N/A                         
  |     C0                                                                                                                                                           
  |                        | 1.4.0 & later     |   64 MB      |  Default Setting            |        Yes        |  N/A                          
  | ------------------------------------------------------------------------------------------------------------------------------------------------------- 

------------
Changes:
------------
1. Fixed Defect 17168 [JER25][PRE CERT][WS2022] USB Exposed Port System Test Fail.
2. Fixed Defect 17173 [JER25][PRE CERT][WS2022] Secure Boot Logo Test Fail.
3. Fixed Defect 17175 [JER25][PRE CERT][WS2022] Hardware Security Testability Interface Test Fail.

*************************************************************************************
* Version:       02.00.00
* System:        JER25 
*   
* Release Date:  10/28/2024
* File Name:     JER25_BIOS_020000.bin 
*
* CRC32 CheckSum: 9FF40BFF
* SHA1  CheckSum: e4394e1b8547117822e0af857d73d6804ba6a09d
* MD5   CheckSum: 7c3e43139aa7046d78f5158146cc3f5c
**************************************************************************************
Integrated module collateral:
 AMI CodeBase:
   Turin:0ACST_PI1.0.0.1_015 (PI 1.0.0.1 / PSP 00.3D.00.65  / SMU 00.5E.6C.00/ U Code (A0 0x0B00004D/B0 0x0B001016/C0 0x0B00202B /C1 0x0B002116/Dense A0 0x0B10000F/Dense B0 0x0B101021)

---------------
Important Note:
---------------
  1.According AMD Doc#58401 Week-5, Update on 64MB SPI chip usage , It limited the BIOS 
    image update method . Please refer BIOS update SOP when boot with Turin ES1/2 CPU.
  2.Installing Windows Server 2019, 2022, or Windows 10, Windows 11, fails with a blue screen of death (BSOD) error and 
    the message "MULTIPROCESSOR CONFIGURATION NOT SUPPORTED" when installing on the listed AMD-based ThinkSystem platforms 
    that have 64+ cores per CPU package. 
   Workaround:
    1. Reduce the CPU core count in UEFI setting System Information -> Processors -> Number of Enabled CPU Cores Per" to 64C before OS installation.
    2. Install Microsoft Windows Server.
    3. Download and apply the latest Windows Monthly Update from Microsoft's website:
    For Win2022:
       https://support.microsoft.com/en-us/topic/windows-server-2022-update-history-e1caa597-00c5-4ab9-9f3e-8212fe80b2ee
    For Win2019:
       https://support.microsoft.com/en-us/topic/windows-10-and-windows-server-2019-update-history-725fc2e1-4443-6831-a5ca-51ff5cbcb059.
  3. After the update installation is completed, reboot the system and re-enable all CPU cores. The OS should then function as expected.
  4. For Windows client OS (Windows 10 or Windows 11), the recommendation is to download and install 22H2 of Windows 11 to support this type of high core count CPUs.
  5. PCIe Root Bridge has exchange from PI 0.0.8.0 . Therefor the Bus number assign has change , (Before: G3=0x20 , P3=0x60 . After: G3=0x60 , P3=0x20)
  6.Enable PFR function , but request PC (C0 stepping) CPU to support it 
  7.Request BMC verison V0.11.0
  8.BIOS start support NMI funciotn , Need to use BMC V0.15.00 to avoid system hang .
-------------
Known Issues:
-------------
  1.BIOS version & CPU stepping matrix trble.
  ---------------------------------------------------------------------------------------------------------------------------------------------------
  |CPU Stepping  |  BIOS Verison  |  Flash Size   |  Prgramming Setting    |  PFR Verify    |  Notice                     
  |                                                                                                                                                                          
  |                        | 1.3.0 & Before  |   32 MB        | Default Setting             |         No        |  N/A                         
  |     A0 / B0                                                                                                                                                           
  |                        | 1.3.0 & Before  |   64 MB        | programming address  |         No        |  N/A                          
  |                                                                         from 0x2000000            |                                                        
  |---------------------------------------------------------------------------------------------------------------------------------------------------
  |                        | 1.4.0 & later     |   32 MB      | Default Setting               |         No        |  N/A                          
  |     A0 / B0                                                                                                                                                        
  |                        | 1.4.0 & later     |   64 MB      | programming address    |         No        |  1.System will random hang during POST
  |                                                                     | from 0x2000000              |         No        |  2.BIOS setup menu value can't chamge  
  |----------------------------------------------------------------------------------------------------------------------------------------------------
  |                        | 1.3.0 & Before  |   32 MB        | Default Setting             |         No        |  System can't boot                    
  |     C0                                                                                                                                                           
  |                        | 1.3.0 & Before  |   64 MB        |  Default Setting            |         No        |   System can't boot                       
  | ------------------------------------------------------------------------------------------------------------------------------------------------------- 
  |                        | 1.4.0 & later     |   32 MB      | Default Setting             |         Yes       |  N/A                         
  |     C0                                                                                                                                                           
  |                        | 1.4.0 & later     |   64 MB      |  Default Setting            |        Yes        |  N/A                          
  | ------------------------------------------------------------------------------------------------------------------------------------------------------- 

------------
Changes:
------------
1. Update PI Code to 1.0.0.1  (Original Version 1.0.0.0)
2. Modify RAS sensor by OEM definition.
3. Implement latest Performance Mode module as A26 Style.

*************************************************************************************
*Version:       01.06.00
*System:        JER25 
*   
*Release Date:  10/07/2024
*File Name:     JER25_BIOS_010600.bin 
*
CRC32 CheckSum: 76a364d8
SHA1  CheckSum: 5a6e1cc6278909e8971944fc777dd20838cc0fa1
MD5   CheckSum: ab418a54fe3d5a4f58cc00f1266bde0b
**************************************************************************************
Integrated module collateral:
 AMI CodeBase:
   Turin:0ACST_PI0.1.0.0RC1 (PI 1.0.0.0 / PSP 00.3D.00.62  / SMU 00.5E.68.00/ U Code (A0 0x0B00004D/B0 0x0B001016/C0 C0 0x0B002024 /C1 C0 0x0B002113/Dense A0 0x0B10000F/Dense B0 0x0B10001D)

---------------
Important Note:
---------------
  1.According AMD Doc#58401 Week-5, Update on 64MB SPI chip usage , It limited the BIOS 
    image update method . Please refer BIOS update SOP when boot with Turin ES1/2 CPU.
  2.Installing Windows Server 2019, 2022, or Windows 10, Windows 11, fails with a blue screen of death (BSOD) error and 
    the message "MULTIPROCESSOR CONFIGURATION NOT SUPPORTED" when installing on the listed AMD-based ThinkSystem platforms 
    that have 64+ cores per CPU package. 
   Workaround:
    1. Reduce the CPU core count in UEFI setting System Information -> Processors -> Number of Enabled CPU Cores Per" to 64C before OS installation.
    2. Install Microsoft Windows Server.
    3. Download and apply the latest Windows Monthly Update from Microsoft's website:
    For Win2022:
       https://support.microsoft.com/en-us/topic/windows-server-2022-update-history-e1caa597-00c5-4ab9-9f3e-8212fe80b2ee
    For Win2019:
       https://support.microsoft.com/en-us/topic/windows-10-and-windows-server-2019-update-history-725fc2e1-4443-6831-a5ca-51ff5cbcb059.
  3. After the update installation is completed, reboot the system and re-enable all CPU cores. The OS should then function as expected.
  4. For Windows client OS (Windows 10 or Windows 11), the recommendation is to download and install 22H2 of Windows 11 to support this type of high core count CPUs.
  5. PCIe Root Bridge has exchange from PI 0.0.8.0 . Therefor the Bus number assign has change , (Before: G3=0x20 , P3=0x60 . After: G3=0x60 , P3=0x20)
  6.Enable PFR function , but request PC (C0 stepping) CPU to support it 
  7.Request BMC verison V0.11.0
  8.BIOS start support NMI funciotn , Need to use BMC V0.15.00 to avoid system hang .
-------------
Known Issues:
-------------
  1.BIOS version & CPU stepping matrix trble.
  ---------------------------------------------------------------------------------------------------------------------------------------------------
  |CPU Stepping  |  BIOS Verison  |  Flash Size   |  Prgramming Setting    |  PFR Verify    |  Notice                     
  |                                                                                                                                                                          
  |                        | 1.3.0 & Before  |   32 MB        | Default Setting             |         No        |  N/A                         
  |     A0 / B0                                                                                                                                                           
  |                        | 1.3.0 & Before  |   64 MB        | programming address  |         No        |  N/A                          
  |                                                                         from 0x2000000            |                                                        
  |---------------------------------------------------------------------------------------------------------------------------------------------------
  |                        | 1.4.0 & later     |   32 MB      | Default Setting               |         No        |  N/A                          
  |     A0 / B0                                                                                                                                                        
  |                        | 1.4.0 & later     |   64 MB      | programming address    |         No        |  1.System will random hang during POST
  |                                                                     | from 0x2000000              |         No        |  2.BIOS setup menu value can't chamge  
  |----------------------------------------------------------------------------------------------------------------------------------------------------
  |                        | 1.3.0 & Before  |   32 MB        | Default Setting             |         No        |  System can't boot                    
  |     C0                                                                                                                                                           
  |                        | 1.3.0 & Before  |   64 MB        |  Default Setting            |         No        |   System can't boot                       
  | ------------------------------------------------------------------------------------------------------------------------------------------------------- 
  |                        | 1.4.0 & later     |   32 MB      | Default Setting             |         Yes       |  N/A                         
  |     C0                                                                                                                                                           
  |                        | 1.4.0 & later     |   64 MB      |  Default Setting            |        Yes        |  N/A                          
  | ------------------------------------------------------------------------------------------------------------------------------------------------------- 
                                          
------------
Changes:
------------
1.Modify BIOS Setup item default (Release JER25_JER15_BIOS_SetupSpec_v0.3).(16940 )
2.Implement RAS sensor to fix unknow sensor issue.(#16789)
3.Remove System event Log menu from BIOS Setup menu .(16852)
4.Update PI Code to 1.0.0
5.Fix system will reboot after hot-plug NVMe under OS.(16633)
6.Fix SMBIOS type-9 information for Slot-6 in SKU3-1 incorrect


*************************************************************************************
*Version:      01.05.00
*System:      JER25 
*              
*Release Date: 09/18/2024
*File Name:    JER25_BIOS_Turin_010500.bin (CRC32 CheckSum: 1b249f69)
**************************************************************************************
Integrated module collateral:
 AMI CodeBase:
   Turin:0ACST_PI0.1.0.0RC1 (PI 1.0.0.0RC1 / PSP 00.3D.00.5E  / SMU 00.5E.5F.00/ U Code (A0 0x0B00004D/B0 0x0B001016/C0 C0 0x0B00201E /C1 C0 0x0B00201E/Dense A0 0x0B10000F/Dense B0 0x0B10000F)

---------------
Important Note:
---------------
  1.According AMD Doc#58401 Week-5, Update on 64MB SPI chip usage , It limited the BIOS 
    image update method . Please refer BIOS update SOP when boot with Turin ES1/2 CPU.
  2.Installing Windows Server 2019, 2022, or Windows 10, Windows 11, fails with a blue screen of death (BSOD) error and 
    the message "MULTIPROCESSOR CONFIGURATION NOT SUPPORTED" when installing on the listed AMD-based ThinkSystem platforms 
    that have 64+ cores per CPU package. 
   Workaround:
    1. Reduce the CPU core count in UEFI setting System Information -> Processors -> Number of Enabled CPU Cores Per" to 64C before OS installation.
    2. Install Microsoft Windows Server.
    3. Download and apply the latest Windows Monthly Update from Microsoft's website:
    For Win2022:
       https://support.microsoft.com/en-us/topic/windows-server-2022-update-history-e1caa597-00c5-4ab9-9f3e-8212fe80b2ee
    For Win2019:
       https://support.microsoft.com/en-us/topic/windows-10-and-windows-server-2019-update-history-725fc2e1-4443-6831-a5ca-51ff5cbcb059.
  3. After the update installation is completed, reboot the system and re-enable all CPU cores. The OS should then function as expected.
  4. For Windows client OS (Windows 10 or Windows 11), the recommendation is to download and install 22H2 of Windows 11 to support this type of high core count CPUs.
  5. PCIe Root Bridge has exchange from PI 0.0.8.0 . Therefor the Bus number assign has change , (Before: G3=0x20 , P3=0x60 . After: G3=0x60 , P3=0x20)
  6.Enable PFR function , but request PC (C0 stepping) CPU to support it 
  7.Request BMC verison V0.11.0
  8.BIOS start support NMI funciotn , Need to use BMC V0.15.00 to avoid system hang .
-------------
Known Issues:
-------------
  1.BIOS version & CPU stepping matrix trble.
  ---------------------------------------------------------------------------------------------------------------------------------------------------
  |CPU Stepping  |  BIOS Verison  |  Flash Size   |  Prgramming Setting    |  PFR Verify    |  Notice                     
  |                                                                                                                                                                          
  |                        | 1.3.0 & Before  |   32 MB        | Default Setting             |         No        |  N/A                         
  |     A0 / B0                                                                                                                                                           
  |                        | 1.3.0 & Before  |   64 MB        | programming address  |         No        |  N/A                          
  |                                                                         from 0x2000000            |                                                        
  |---------------------------------------------------------------------------------------------------------------------------------------------------
  |                        | 1.4.0 & later     |   32 MB      | Default Setting               |         No        |  N/A                          
  |     A0 / B0                                                                                                                                                        
  |                        | 1.4.0 & later     |   64 MB      | programming address    |         No        |  1.System will random hang during POST
  |                                                                     | from 0x2000000              |         No        |  2.BIOS setup menu value can't chamge  
  |----------------------------------------------------------------------------------------------------------------------------------------------------
  |                        | 1.3.0 & Before  |   32 MB        | Default Setting             |         No        |  System can't boot                    
  |     C0                                                                                                                                                           
  |                        | 1.3.0 & Before  |   64 MB        |  Default Setting            |         No        |   System can't boot                       
  | ------------------------------------------------------------------------------------------------------------------------------------------------------- 
  |                        | 1.4.0 & later     |   32 MB      | Default Setting             |         Yes       |  N/A                         
  |     C0                                                                                                                                                           
  |                        | 1.4.0 & later     |   64 MB      |  Default Setting            |        Yes        |  N/A                          
  | ------------------------------------------------------------------------------------------------------------------------------------------------------- 
                                          
------------
Changes:
------------
1.Enable Secure Boot function (Import PK/KEK keys).
2.Enable Performance item in Setup menu.
3.Modify SMBIOS TYPE8.Internal connector to External connector .
   (Reference type-8 example in SMBIOS Spec)
4.Modify SMBIOS TYPE9.SlotLength to Long.


*************************************************************************************
*Version:      01.04.00
*System:       JER15 / JER25 
*              
*Release Date: 09/02/2024
*File Name:    JER25_BIOS_Turin_010400bin (CRC32 CheckSum: a4342141 )
**************************************************************************************
Integrated module collateral:
 AMI CodeBase:
   Turin:0ACST_PI0.1.0.0RC1 (PI 1.0.0.0RC1 / PSP 00.3D.00.5E  / SMU 00.5E.5F.00/ U Code (A0 0x0B00004D/B0 0x0B001016/C0 C0 0x0B00201E /C1 C0 0x0B00201E/Dense A0 0x0B10000F/Dense B0 0x0B10000F)

---------------
Important Note:
---------------
  1.According AMD Doc#58401 Week-5, Update on 64MB SPI chip usage , It limited the BIOS 
    image update method . Please refer BIOS update SOP when boot with Turin ES1/2 CPU.
  2.Installing Windows Server 2019, 2022, or Windows 10, Windows 11, fails with a blue screen of death (BSOD) error and 
    the message "MULTIPROCESSOR CONFIGURATION NOT SUPPORTED" when installing on the listed AMD-based ThinkSystem platforms 
    that have 64+ cores per CPU package. 
   Workaround:
    1. Reduce the CPU core count in UEFI setting System Information -> Processors -> Number of Enabled CPU Cores Per" to 64C before OS installation.
    2. Install Microsoft Windows Server.
    3. Download and apply the latest Windows Monthly Update from Microsoft's website:
    For Win2022:
       https://support.microsoft.com/en-us/topic/windows-server-2022-update-history-e1caa597-00c5-4ab9-9f3e-8212fe80b2ee
    For Win2019:
       https://support.microsoft.com/en-us/topic/windows-10-and-windows-server-2019-update-history-725fc2e1-4443-6831-a5ca-51ff5cbcb059.
  3. After the update installation is completed, reboot the system and re-enable all CPU cores. The OS should then function as expected.
  4. For Windows client OS (Windows 10 or Windows 11), the recommendation is to download and install 22H2 of Windows 11 to support this type of high core count CPUs.
  5. PCIe Root Bridge has exchange from PI 0.0.8.0 . Therefor the Bus number assign has change , (Before: G3=0x20 , P3=0x60 . After: G3=0x60 , P3=0x20)
  6.Enable PFR function , but request PC (C0 stepping) CPU to support it 
  7.Request BMC verison V0.11.0
  8.BIOS start support NMI funciotn , Need to use BMC V0.15.00 to avoid system hang .
-------------
Known Issues:
-------------
  1.BIOS version & CPU stepping matrix trble.
  ---------------------------------------------------------------------------------------------------------------------------------------------------
  |CPU Stepping  |  BIOS Verison  |  Flash Size   |  Prgramming Setting    |  PFR Verify    |  Notice                     
  |                                                                                                                                                                          
  |                        | 1.3.0 & Before  |   32 MB        | Default Setting             |         No        |  N/A                         
  |     A0 / B0                                                                                                                                                           
  |                        | 1.3.0 & Before  |   64 MB        | programming address         |         No        |  N/A                          
  |                                                             from 0x2000000              |                                                        
  |---------------------------------------------------------------------------------------------------------------------------------------------------
  |                        | 1.4.0 & later     |   32 MB      | Default Setting             |         No        |  N/A                          
  |     A0 / B0                                                                                                                                                        
  |                        | 1.4.0 & later     |   64 MB      | programming address         |         No        |  1.System will random hang during POST
  |                                                           | from 0x2000000              |         No        |  2.BIOS setup menu value can't chamge  
  |----------------------------------------------------------------------------------------------------------------------------------------------------
  |                        | 1.3.0 & Before  |   32 MB        | Default Setting             |         No        |  System can't boot                    
  |     C0                                                                                                                                                           
  |                        | 1.3.0 & Before  |   64 MB        |  Default Setting            |         No        |   System can't boot                       
  | ------------------------------------------------------------------------------------------------------------------------------------------------------- 
  |                        | 1.4.0 & later     |   32 MB      | Default Setting             |         Yes       |  N/A                         
  |     C0                                                                                                                                                           
  |                        | 1.4.0 & later     |   64 MB      |  Default Setting            |        Yes        |  N/A                          
  | ------------------------------------------------------------------------------------------------------------------------------------------------------- 
                                          
------------
Changes:
------------
1.Enable SOL function.
2.Fix DF-16338_1 The “dmidecode –t 9” does not show PCIe slot 1 information for SKU4 & SKU4-1  
3.Fix DF-15749_1 FIO USB over current test_POST no warning, SEL doesn't show USB OCP warning log 


*************************************************************************************
*Version:      01.03.00
*System:       JER15 / JER25 
*              
*Release Date: 08/19/2024
*File Name:    JER25_BIOS_Turin_010200bin (CRC32 CheckSum: 686aa93c )
**************************************************************************************
Integrated module collateral:
 AMI CodeBase:
   Turin:0ACST_PI0.1.0.0RC1 (PI 1.0.0.0RC1 / PSP 00.3D.00.5E  / SMU 00.5E.5F.00/ U Code (A0 0x0B00004D/B0 0x0B001016/C0 C0 0x0B00201E /C1 C0 0x0B00201E/Dense A0 0x0B10000F/Dense B0 0x0B10000F)

---------------
Important Note:
---------------
  1.According AMD Doc#58401 Week-5, Update on 64MB SPI chip usage , It limited the BIOS 
    image update method . Please refer BIOS update SOP when boot with Turin ES1/2 CPU.
  2.Installing Windows Server 2019, 2022, or Windows 10, Windows 11, fails with a blue screen of death (BSOD) error and 
    the message "MULTIPROCESSOR CONFIGURATION NOT SUPPORTED" when installing on the listed AMD-based ThinkSystem platforms 
    that have 64+ cores per CPU package. 
   Workaround:
    1. Reduce the CPU core count in UEFI setting System Information -> Processors -> Number of Enabled CPU Cores Per" to 64C before OS installation.
    2. Install Microsoft Windows Server.
    3. Download and apply the latest Windows Monthly Update from Microsoft's website:
    For Win2022:
       https://support.microsoft.com/en-us/topic/windows-server-2022-update-history-e1caa597-00c5-4ab9-9f3e-8212fe80b2ee
    For Win2019:
       https://support.microsoft.com/en-us/topic/windows-10-and-windows-server-2019-update-history-725fc2e1-4443-6831-a5ca-51ff5cbcb059.
  3. After the update installation is completed, reboot the system and re-enable all CPU cores. The OS should then function as expected.
  4. For Windows client OS (Windows 10 or Windows 11), the recommendation is to download and install 22H2 of Windows 11 to support this type of high core count CPUs.
  5. PCIe Root Bridge has exchange from PI 0.0.8.0 . Therefor the Bus number assign has change , (Before: G3=0x20 , P3=0x60 . After: G3=0x60 , P3=0x20)
  6.Enable PFR function , but request PC (C0 stepping) CPU to support it 
  7.Request BMC verison V0.11.0
  8.BIOS start support NMI funciotn , Need to use BMC V0.15.00 to avoid system hang .
-------------
Known Issues:
-------------
  1.BIOS version & CPU stepping matrix trble.
  ---------------------------------------------------------------------------------------------------------------------------------------------------
  |CPU Stepping  |  BIOS Verison  |  Flash Size   |  Prgramming Setting    |  PFR Verify    |  Notice                     
  |                                                                                                                                                                          
  |                        | 1.3.0 & Before  |   32 MB        | Default Setting             |         No        |  N/A                         
  |     A0 / B0                                                                                                                                                           
  |                        | 1.3.0 & Before  |   64 MB        | programming address         |         No        |  N/A                          
  |                                                             from 0x2000000              |                                                        
  |---------------------------------------------------------------------------------------------------------------------------------------------------
  |                        | 1.4.0 & later     |   32 MB      | Default Setting             |         No        |  N/A                          
  |     A0 / B0                                                                                                                                                        
  |                        | 1.4.0 & later     |   64 MB      | programming address         |         No        |  1.System will random hang during POST
  |                                                           | from 0x2000000              |         No        |  2.BIOS setup menu value can't chamge  
  |----------------------------------------------------------------------------------------------------------------------------------------------------
  |                        | 1.3.0 & Before  |   32 MB        | Default Setting             |         No        |  System can't boot                    
  |     C0                                                                                                                                                           
  |                        | 1.3.0 & Before  |   64 MB        |  Default Setting            |         No        |   System can't boot                       
  | ------------------------------------------------------------------------------------------------------------------------------------------------------- 
  |                        | 1.4.0 & later     |   32 MB      | Default Setting             |         Yes       |  N/A                         
  |     C0                                                                                                                                                           
  |                        | 1.4.0 & later     |   64 MB      |  Default Setting            |        Yes        |  N/A                          
  | ------------------------------------------------------------------------------------------------------------------------------------------------------- 
                                          
------------
Changes:
------------
1.[DF16395] SMBIOS_Typr 16/17 of Error Information Handle value is incorrect.
2.Move NVMe f/w interface under NVMe submenu.
3.Support SOL from BMC V.0.  .
4.[DF16517] Fix "SMBIOS_Typr 9" slot information "Data Bus Width" value incorrect when install X16 PCIe card in all SKU. 
5.Add Shared Nic information during POST screen.

*************************************************************************************
*Version:      01.02.00
*System:       JER15 / JER25 
*              
*Release Date: 08/05/2024
*File Name:    JER25_BIOS_Turin_010200bin (CRC32 CheckSum: a4236958 )
**************************************************************************************
Integrated module collateral:
 AMI CodeBase:
   Turin:0ACST_PI0.1.0.0RC1 (PI 1.0.0.0RC1 / PSP 00.3D.00.5E  / SMU 00.5E.5F.00/ U Code (A0 0x0B00004D/B0 0x0B001016/C0 C0 0x0B00201E /C1 C0 0x0B00201E/Dense A0 0x0B10000F/Dense B0 0x0B10000F)

---------------
Important Note:
---------------
  1.According AMD Doc#58401 Week-5, Update on 64MB SPI chip usage , It limited the BIOS 
    image update method . Please refer BIOS update SOP when boot with Turin ES1/2 CPU.
  2.Installing Windows Server 2019, 2022, or Windows 10, Windows 11, fails with a blue screen of death (BSOD) error and 
    the message "MULTIPROCESSOR CONFIGURATION NOT SUPPORTED" when installing on the listed AMD-based ThinkSystem platforms 
    that have 64+ cores per CPU package. 
   Workaround:
    1. Reduce the CPU core count in UEFI setting System Information -> Processors -> Number of Enabled CPU Cores Per" to 64C before OS installation.
    2. Install Microsoft Windows Server.
    3. Download and apply the latest Windows Monthly Update from Microsoft's website:
    For Win2022:
       https://support.microsoft.com/en-us/topic/windows-server-2022-update-history-e1caa597-00c5-4ab9-9f3e-8212fe80b2ee
    For Win2019:
       https://support.microsoft.com/en-us/topic/windows-10-and-windows-server-2019-update-history-725fc2e1-4443-6831-a5ca-51ff5cbcb059.
  3. After the update installation is completed, reboot the system and re-enable all CPU cores. The OS should then function as expected.
  4. For Windows client OS (Windows 10 or Windows 11), the recommendation is to download and install 22H2 of Windows 11 to support this type of high core count CPUs.
  5. PCIe Root Bridge has exchange from PI 0.0.8.0 . Therefor the Bus number assign has change , (Before: G3=0x20 , P3=0x60 . After: G3=0x60 , P3=0x20)
  6.Enable PFR function , but request PC (C0 stepping) CPU to support it 
  7.Request BMC verison V0.11.0
-------------
Known Issues:
-------------
   1.BIOS 0.1.4 can't save setup menu change when use 64 MB Rom part , Suggest change to 32 MB Rom part. 
   2.Rear USB Prt will random fail from BIOS 0.1.4
   3.System will random hang when use 64 MB Rom part , Suggest change to 32 MB Rom part.  
   4.BIOS version & CPU stepping matrix trble.
  ---------------------------------------------------------------------------------------------------------------------------------------------------
  |CPU Stepping  |  BIOS Verison  |  Flash Size   |  Prgramming Setting    |  PFR Verify   |  Notice                     
  |                                                                                                                                                                          
  |                        | 1.3.0 & Before  |   32 MB        | Default Setting             |         No        |  N/A                         
  |     A0 / B0                                                                                                                                                           
  |                        | 1.3.0 & Before  |   64 MB        | programming address  |         No        |  N/A                          
  |                                                                          from 0x2000000           |                                                        
  |---------------------------------------------------------------------------------------------------------------------------------------------------
  |                        | 1.4.0 & later     |   32 MB        | Default Setting             |         No        |  N/A                          
  |     A0 / B0                                                                                                                                                        
  |                        | 1.4.0 & later     |   64 MB        | programming address  |         No        |  1.System will random hang during POST
  |                                                                       | from 0x2000000            |         No        |  2.BIOS setup menu value can't chamge  
  |----------------------------------------------------------------------------------------------------------------------------------------------------
  |                        | 1.3.0 & Before  |   32 MB        | Default Setting             |         No        |  System can't boot                    
  |     C0                                                                                                                                                           
  |                        | 1.3.0 & Before  |   64 MB        |  Default Setting            |         No        |   System can't boot                       
  | ------------------------------------------------------------------------------------------------------------------------------------------------------- 
  |                        | 1.4.0 & later     |   32 MB        | Default Setting             |         Yes       |  N/A                         
  |     C0                                                                                                                                                           
  |                        | 1.4.0 & later     |   64 MB        |  Default Setting            |        Yes        |  N/A                          
  | ------------------------------------------------------------------------------------------------------------------------------------------------------- 
   5.SKU:2-1 & 4-1 configuration not support yet .  

                                          
------------
Changes:
------------
1.Modify SKU 1 & 1-1 Slot number.
2.[DF15886] Modify PCIe Oem porting interface.
3.Enable PspEarlyVga.
4.Fix build error fo FRU SMBIOS hang 0x62 solution.
5.Fix no Data Bus Width in SMBIOS type-9.
6.Fix [DF16327] One of NVME can't be detected on rear 2HDD, SKU1-1 (include SKU 3-1 / 4-1).
7.Add new riser bifurcation setting for SC-A239P_RISER.
8.SMBIOS type-9 information no list Slot-1 & Slot-2 in SKU 1-1 . 
9.Update AMD Codebase  to PI-1.0.0.0 RC1


*************************************************************************************
*Version:      01.01.00
*System:       JER15 / JER25 
*              
*Release Date: 07/21/2024
*File Name:    JER25_BIOS_Turin_000108bin (CRC32 CheckSum: 09540fce )
**************************************************************************************
Integrated module collateral:
 AMI CodeBase:
   Turin:0ACST_PI0.0.9.0 (PI 0.0.9.0 / PSP 00.3D.00.5B / SMU 00.5E.5B.00/ U Code (A0 0x0B00004D/B0 0x0B001016/C0 0x0B00201D /C1 0X0B002109/Dense A0 0xB10000F/Dense B0 0xB10100E)

---------------
Important Note:
---------------
  1.According AMD Doc#58401 Week-5, Update on 64MB SPI chip usage , It limited the BIOS 
    image update method . Please refer BIOS update SOP when boot with Turin ES1/2 CPU.
  2.Installing Windows Server 2019, 2022, or Windows 10, Windows 11, fails with a blue screen of death (BSOD) error and 
    the message "MULTIPROCESSOR CONFIGURATION NOT SUPPORTED" when installing on the listed AMD-based ThinkSystem platforms 
    that have 64+ cores per CPU package. 
   Workaround:
    1. Reduce the CPU core count in UEFI setting System Information -> Processors -> Number of Enabled CPU Cores Per" to 64C before OS installation.
    2. Install Microsoft Windows Server.
    3. Download and apply the latest Windows Monthly Update from Microsoft's website:
    For Win2022:
       https://support.microsoft.com/en-us/topic/windows-server-2022-update-history-e1caa597-00c5-4ab9-9f3e-8212fe80b2ee
    For Win2019:
       https://support.microsoft.com/en-us/topic/windows-10-and-windows-server-2019-update-history-725fc2e1-4443-6831-a5ca-51ff5cbcb059.
  3. After the update installation is completed, reboot the system and re-enable all CPU cores. The OS should then function as expected.
  4. For Windows client OS (Windows 10 or Windows 11), the recommendation is to download and install 22H2 of Windows 11 to support this type of high core count CPUs.
  5. PCIe Root Bridge has exchange from PI 0.0.8.0 . Therefor the Bus number assign has change , (Before: G3=0x20 , P3=0x60 . After: G3=0x60 , P3=0x20)
  6.Enable PFR function , but request PC (C0 stepping) CPU to support it 
  7.Request BMC verison V0.11.0
-------------
Known Issues:
-------------
   1.BIOS 0.1.4 can't save setup menu change when use 64 MB Rom part , Suggest change to 32 MB Rom part. 
   2.Rear USB Prt will random fail from BIOS 0.1.4
   3.System will random hang when use 64 MB Rom part , Suggest change to 32 MB Rom part.  
   4.BIOS version & CPU stepping matrix trble.
  ---------------------------------------------------------------------------------------------------------------------------------------------------
  |CPU Stepping  |  BIOS Verison  |  Flash Size   |  Prgramming Setting    |  PFR Verify   |  Notice                     
  |                                                                                                                                                                          
  |                        | 1.3.0 & Before  |   32 MB        | Default Setting             |         No        |  N/A                         
  |     A0 / B0                                                                                                                                                           
  |                        | 1.3.0 & Before  |   64 MB        | programming address  |         No        |  N/A                          
  |                                                                          from 0x2000000           |                                                        
  |---------------------------------------------------------------------------------------------------------------------------------------------------
  |                        | 1.4.0 & later     |   32 MB        | Default Setting             |         No        |  N/A                          
  |     A0 / B0                                                                                                                                                        
  |                        | 1.4.0 & later     |   64 MB        | programming address  |         No        |  1.System will random hang during POST
  |                                                                       | from 0x2000000            |         No        |  2.BIOS setup menu value can't chamge  
  |----------------------------------------------------------------------------------------------------------------------------------------------------
  |                        | 1.3.0 & Before  |   32 MB        | Default Setting             |         No        |  System can't boot                    
  |     C0                                                                                                                                                           
  |                        | 1.3.0 & Before  |   64 MB        |  Default Setting            |         No        |   System can't boot                       
  | ------------------------------------------------------------------------------------------------------------------------------------------------------- 
  |                        | 1.4.0 & later     |   32 MB        | Default Setting             |         Yes       |  N/A                         
  |     C0                                                                                                                                                           
  |                        | 1.4.0 & later     |   64 MB        |  Default Setting            |        Yes        |  N/A                          
  | ------------------------------------------------------------------------------------------------------------------------------------------------------- 
   5.SKU:2-1 & 4-1 configuration not support yet .  

                                          
------------
Changes:
------------
1.Fix [16338] [DVT]The “dmidecode –t 9” does not show PCIe slot 1 information.
2.Fix [16327] [JER25][DVT]One of NVME can't be detected on rear 2HDD, SKU1-1





*************************************************************************************
*Version:      01.00.00
*System:       JER15 / JER25 
*              
*Release Date: 07/08/2024
*File Name:    JER25_BIOS_Turin_000108bin (CRC32 CheckSum: 09540fce )
**************************************************************************************
Integrated module collateral:
 AMI CodeBase:
   Turin:0ACST_PI0.0.9.0 (PI 0.0.9.0 / PSP 00.3D.00.5B / SMU 00.5E.5B.00/ U Code (A0 0x0B00004D/B0 0x0B001016/C0 0x0B00201D /C1 0X0B002109/Dense A0 0xB10000F/Dense B0 0xB10100E)

---------------
Important Note:
---------------
  1.According AMD Doc#58401 Week-5, Update on 64MB SPI chip usage , It limited the BIOS 
    image update method . Please refer BIOS update SOP when boot with Turin ES1/2 CPU.
  2.Installing Windows Server 2019, 2022, or Windows 10, Windows 11, fails with a blue screen of death (BSOD) error and 
    the message "MULTIPROCESSOR CONFIGURATION NOT SUPPORTED" when installing on the listed AMD-based ThinkSystem platforms 
    that have 64+ cores per CPU package. 
   Workaround:
    1. Reduce the CPU core count in UEFI setting System Information -> Processors -> Number of Enabled CPU Cores Per" to 64C before OS installation.
    2. Install Microsoft Windows Server.
    3. Download and apply the latest Windows Monthly Update from Microsoft's website:
    For Win2022:
       https://support.microsoft.com/en-us/topic/windows-server-2022-update-history-e1caa597-00c5-4ab9-9f3e-8212fe80b2ee
    For Win2019:
       https://support.microsoft.com/en-us/topic/windows-10-and-windows-server-2019-update-history-725fc2e1-4443-6831-a5ca-51ff5cbcb059.
  3. After the update installation is completed, reboot the system and re-enable all CPU cores. The OS should then function as expected.
  4. For Windows client OS (Windows 10 or Windows 11), the recommendation is to download and install 22H2 of Windows 11 to support this type of high core count CPUs.
  5. PCIe Root Bridge has exchange from PI 0.0.8.0 . Therefor the Bus number assign has change , (Before: G3=0x20 , P3=0x60 . After: G3=0x60 , P3=0x20)
  6.Enable PFR function , but request PC (C0 stepping) CPU to support it 
  7.Request BMC verison V0.11.0
-------------
Known Issues:
-------------
   1.BIOS 0.1.4 can't save setup menu change when use 64 MB Rom part , Suggest change to 32 MB Rom part. 
   2.Rear USB Prt will random fail from BIOS 0.1.4
   3.System will random hang when use 64 MB Rom part , Suggest change to 32 MB Rom part.  
   4.BIOS version & CPU stepping matrix trble.
  ---------------------------------------------------------------------------------------------------------------------------------------------------
  |CPU Stepping  |  BIOS Verison  |  Flash Size   |  Prgramming Setting    |  PFR Verify   |  Notice                     
  |                                                                                                                                                                          
  |                        | 1.3.0 & Before  |   32 MB        | Default Setting             |         No        |  N/A                         
  |     A0 / B0                                                                                                                                                           
  |                        | 1.3.0 & Before  |   64 MB        | programming address  |         No        |  N/A                          
  |                                                                          from 0x2000000           |                                                        
  |---------------------------------------------------------------------------------------------------------------------------------------------------
  |                        | 1.4.0 & later     |   32 MB        | Default Setting             |         No        |  N/A                          
  |     A0 / B0                                                                                                                                                        
  |                        | 1.4.0 & later     |   64 MB        | programming address  |         No        |  1.System will random hang during POST
  |                                                                       | from 0x2000000            |         No        |  2.BIOS setup menu value can't chamge  
  |----------------------------------------------------------------------------------------------------------------------------------------------------
  |                        | 1.3.0 & Before  |   32 MB        | Default Setting             |         No        |  System can't boot                    
  |     C0                                                                                                                                                           
  |                        | 1.3.0 & Before  |   64 MB        |  Default Setting            |         No        |   System can't boot                       
  | ------------------------------------------------------------------------------------------------------------------------------------------------------- 
  |                        | 1.4.0 & later     |   32 MB        | Default Setting             |         Yes       |  N/A                         
  |     C0                                                                                                                                                           
  |                        | 1.4.0 & later     |   64 MB        |  Default Setting            |        Yes        |  N/A                          
  | ------------------------------------------------------------------------------------------------------------------------------------------------------- 
   5.SKU:2-1 & 4-1 configuration not support yet .  

                                          
------------
Changes:
------------
1.Expose Core Performance Boost due to 500 CPU will cause system hang up. 
2.Update PI Version to 0.0.9.0.
3.Fix rear USB OC trigger condition.
4.Fix NVMe device sequence under OS.


*************************************************************************************
*Version:      00.01.08
*System:       JER15 / JER25 
*              
*Release Date: 06/11/2024
*File Name:    JER25_BIOS_Turin_000108bin (CRC32 CheckSum: 09540fce )
**************************************************************************************
Integrated module collateral:
 AMI CodeBase:
   Turin:0ACST_PI0.0.8.1 (PI 0.0.8.1 / PSP 00.3D.00.55 / SMU 00.5E.53.64/ U Code (A0 0x0B000048/B0 0x0B001014/C0 0x0B00200E /C1 0X0B002102/Dense A0 0xB10000F/Dense B0 0xB101003)

---------------
Important Note:
---------------
  1.According AMD Doc#58401 Week-5, Update on 64MB SPI chip usage , It limited the BIOS 
    image update method . Please refer BIOS update SOP when boot with Turin ES1/2 CPU.
  2.Installing Windows Server 2019, 2022, or Windows 10, Windows 11, fails with a blue screen of death (BSOD) error and 
    the message "MULTIPROCESSOR CONFIGURATION NOT SUPPORTED" when installing on the listed AMD-based ThinkSystem platforms 
    that have 64+ cores per CPU package. 
   Workaround:
    1. Reduce the CPU core count in UEFI setting System Information -> Processors -> Number of Enabled CPU Cores Per" to 64C before OS installation.
    2. Install Microsoft Windows Server.
    3. Download and apply the latest Windows Monthly Update from Microsoft's website:
    For Win2022:
       https://support.microsoft.com/en-us/topic/windows-server-2022-update-history-e1caa597-00c5-4ab9-9f3e-8212fe80b2ee
    For Win2019:
       https://support.microsoft.com/en-us/topic/windows-10-and-windows-server-2019-update-history-725fc2e1-4443-6831-a5ca-51ff5cbcb059.
  3. After the update installation is completed, reboot the system and re-enable all CPU cores. The OS should then function as expected.
  4. For Windows client OS (Windows 10 or Windows 11), the recommendation is to download and install 22H2 of Windows 11 to support this type of high core count CPUs.
  5. PCIe Root Bridge has exchange from PI 0.0.8.0 . Therefor the Bus number assign has change , (Before: G3=0x20 , P3=0x60 . After: G3=0x60 , P3=0x20)
  6.Enable PFR function , but request PC (C0 stepping) CPU to support it 
  7.Request BMC verison V0.11.0
-------------
Known Issues:
-------------
   1.BIOS 0.1.4 can't save setup menu change when use 64 MB Rom part , Suggest change to 32 MB Rom part. 
   2.Rear USB Prt will random fail from BIOS 0.1.4
   3.System will random hang when use 64 MB Rom part , Suggest change to 32 MB Rom part.  
   4.BIOS version & CPU stepping matrix trble.
  ---------------------------------------------------------------------------------------------------------------------------------------------------
  |CPU Stepping  |  BIOS Verison  |  Flash Size   |  Prgramming Setting    |  PFR Verify   |  Notice                     
  |                                                                                                                                                                          
  |                        | 1.3.0 & Before  |   32 MB        | Default Setting             |         No        |  N/A                         
  |     A0 / B0                                                                                                                                                           
  |                        | 1.3.0 & Before  |   64 MB        | programming address  |         No        |  N/A                          
  |                                                                          from 0x2000000           |                                                        
  |---------------------------------------------------------------------------------------------------------------------------------------------------
  |                        | 1.4.0 & later     |   32 MB        | Default Setting             |         No        |  N/A                          
  |     A0 / B0                                                                                                                                                        
  |                        | 1.4.0 & later     |   64 MB        | programming address  |         No        |  1.System will random hang during POST
  |                                                                       | from 0x2000000            |         No        |  2.BIOS setup menu value can't chamge  
  |----------------------------------------------------------------------------------------------------------------------------------------------------
  |                        | 1.3.0 & Before  |   32 MB        | Default Setting             |         No        |  System can't boot                    
  |     C0                                                                                                                                                           
  |                        | 1.3.0 & Before  |   64 MB        |  Default Setting            |         No        |   System can't boot                       
  | ------------------------------------------------------------------------------------------------------------------------------------------------------- 
  |                        | 1.4.0 & later     |   32 MB        | Default Setting             |         Yes       |  N/A                         
  |     C0                                                                                                                                                           
  |                        | 1.4.0 & later     |   64 MB        |  Default Setting            |        Yes        |  N/A                          
  | -------------------------------------------------------------------------------------------------------------------------------------------------------                                          
------------
Changes:
------------
1.Fix EIP-799512 Press Ctrl_Alt_Del key to reboot system will delay around 5-10 seconds when add System Inventory funciton. 
2.Add PCIe Oem porting interface for new configuration support.
3.Update checking condition to detection USB Over current for [15725/15726] [JER15/25] Add debug log for USB over current warning function analysis
4.Add KER45 (MTK) Sku.



*************************************************************************************
*Version:      00.01.07
*System:       JER15 / JER25 
*              
*Release Date: 05/24/2024
*File Name:    JER25_BIOS_Turin_000107bin (CRC32 CheckSum:AEC8DAF0)
**************************************************************************************
Integrated module collateral:
 AMI CodeBase:
   Turin:0ACST_PI0.0.8.1 (PI 0.0.8.1 / PSP 00.3D.00.55 / SMU 00.5E.53.64/ U Code (A0 0x0B000048/B0 0x0B001014/C0 0x0B00200E /C1 0X0B002102/Dense A0 0xB10000F/Dense B0 0xB101003)

---------------
Important Note:
---------------
  1.According AMD Doc#58401 Week-5, Update on 64MB SPI chip usage , It limited the BIOS 
    image update method . Please refer BIOS update SOP when boot with Turin ES1/2 CPU.
  2.Installing Windows Server 2019, 2022, or Windows 10, Windows 11, fails with a blue screen of death (BSOD) error and 
    the message "MULTIPROCESSOR CONFIGURATION NOT SUPPORTED" when installing on the listed AMD-based ThinkSystem platforms 
    that have 64+ cores per CPU package. 
   Workaround:
    1. Reduce the CPU core count in UEFI setting System Information -> Processors -> Number of Enabled CPU Cores Per" to 64C before OS installation.
    2. Install Microsoft Windows Server.
    3. Download and apply the latest Windows Monthly Update from Microsoft's website:
    For Win2022:
       https://support.microsoft.com/en-us/topic/windows-server-2022-update-history-e1caa597-00c5-4ab9-9f3e-8212fe80b2ee
    For Win2019:
       https://support.microsoft.com/en-us/topic/windows-10-and-windows-server-2019-update-history-725fc2e1-4443-6831-a5ca-51ff5cbcb059.
  3. After the update installation is completed, reboot the system and re-enable all CPU cores. The OS should then function as expected.
  4. For Windows client OS (Windows 10 or Windows 11), the recommendation is to download and install 22H2 of Windows 11 to support this type of high core count CPUs.
  5. PCIe Root Bridge has exchange from PI 0.0.8.0 . Therefor the Bus number assign has change , (Before: G3=0x20 , P3=0x60 . After: G3=0x60 , P3=0x20)
  6.Enable PFR function , but request PC (C0 stepping) CPU to support it 
  7.Request BMC verison V0.11.0
-------------
Known Issues:
-------------
   1.BIOS 0.1.4 can't save setup menu change when use 64 MB Rom part , Suggest change to 32 MB Rom part. 
   2.Rear USB Prt will random fail from BIOS 0.1.4
   3.System will random hang when use 64 MB Rom part , Suggest change to 32 MB Rom part.  
   4.BIOS version & CPU stepping matrix trble.
  ---------------------------------------------------------------------------------------------------------------------------------------------------
  |CPU Stepping  |  BIOS Verison  |  Flash Size   |  Prgramming Setting    |  PFR Verify   |  Notice                     
  |                                                                                                                                                                          
  |                        | 1.3.0 & Before  |   32 MB        | Default Setting             |         No        |  N/A                         
  |     A0 / B0                                                                                                                                                           
  |                        | 1.3.0 & Before  |   64 MB        | programming address  |         No        |  N/A                          
  |                                                                          from 0x2000000           |                                                        
  |---------------------------------------------------------------------------------------------------------------------------------------------------
  |                        | 1.4.0 & later     |   32 MB        | Default Setting             |         No        |  N/A                          
  |     A0 / B0                                                                                                                                                        
  |                        | 1.4.0 & later     |   64 MB        | programming address  |         No        |  1.System will random hang during POST
  |                                                                       | from 0x2000000            |         No        |  2.BIOS setup menu value can't chamge  
  |----------------------------------------------------------------------------------------------------------------------------------------------------
  |                        | 1.3.0 & Before  |   32 MB        | Default Setting             |         No        |  System can't boot                    
  |     C0                                                                                                                                                           
  |                        | 1.3.0 & Before  |   64 MB        |  Default Setting            |         No        |   System can't boot                       
  | ------------------------------------------------------------------------------------------------------------------------------------------------------- 
  |                        | 1.4.0 & later     |   32 MB        | Default Setting             |         Yes       |  N/A                         
  |     C0                                                                                                                                                           
  |                        | 1.4.0 & later     |   64 MB        |  Default Setting            |        Yes        |  N/A                          
  | -------------------------------------------------------------------------------------------------------------------------------------------------------                                          
------------
Changes:
------------
1.New HDD BP ID support , Need to use BMC V.11 to support new configuration . 
2.[JER15/25][EVT] POST show "USB Port over current detected"message randomly during boot time.
3.[159550] [JER15/25][EVT] USB device not detected during reboot/DC cycle.
4.Fix-[JER15/JER25] RedFish lost module part
5.[JER15/25] CRB12_PI0.0.8.1 codebase update



*************************************************************************************
*Version:      00.01.06
*System:       JER15 / JER25 
*              
*Release Date: 05/10/2024
*File Name:    JER25_BIOS_Turin_000106bin
**************************************************************************************
Integrated module collateral:
 AMI CodeBase:
   Turin:0ACST_PI0.0.8.0 (PI 0.0.8.0 / PSP 00.3D.00.52 / SMU 00.5E.4F.00 / U Code (A0 0x0B000048/B0 0x0B001014/C0 0x0B002006 /Dense A0 0xB100008)

---------------
Important Note:
---------------
  1.According AMD Doc#58401 Week-5, Update on 64MB SPI chip usage , It limited the BIOS 
    image update method . Please refer BIOS update SOP when boot with Turin ES1/2 CPU.
  2.Installing Windows Server 2019, 2022, or Windows 10, Windows 11, fails with a blue screen of death (BSOD) error and 
    the message "MULTIPROCESSOR CONFIGURATION NOT SUPPORTED" when installing on the listed AMD-based ThinkSystem platforms 
    that have 64+ cores per CPU package. 
   Workaround:
    1. Reduce the CPU core count in UEFI setting System Information -> Processors -> Number of Enabled CPU Cores Per" to 64C before OS installation.
    2. Install Microsoft Windows Server.
    3. Download and apply the latest Windows Monthly Update from Microsoft's website:
    For Win2022:
       https://support.microsoft.com/en-us/topic/windows-server-2022-update-history-e1caa597-00c5-4ab9-9f3e-8212fe80b2ee
    For Win2019:
       https://support.microsoft.com/en-us/topic/windows-10-and-windows-server-2019-update-history-725fc2e1-4443-6831-a5ca-51ff5cbcb059.
  3. After the update installation is completed, reboot the system and re-enable all CPU cores. The OS should then function as expected.
  4. For Windows client OS (Windows 10 or Windows 11), the recommendation is to download and install 22H2 of Windows 11 to support this type of high core count CPUs.
  5. PCIe Root Bridge has exchange from PI 0.0.8.0 . Therefor the Bus number assign has change , (Before: G3=0x20 , P3=0x60 . After: G3=0x60 , P3=0x20)
  6.Enable PFR function , but request PC (C0 stepping) CPU to support it 
-------------
Known Issues:
-------------
   1.BIOS 0.1.4 can't save setup menu change when use 64 MB Rom part , Suggest change to 32 MB Rom part. 
   2.Rear USB Prt will random fail from BIOS 0.1.4
   3.System will random hang when use 64 MB Rom part , Suggest change to 32 MB Rom part.  
   4.BIOS version & CPU stepping matrix trble.
  ---------------------------------------------------------------------------------------------------------------------------------------------------
  |CPU Stepping  |  BIOS Verison  |  Flash Size   |  Prgramming Setting    |  PFR Verify   |  Notice                     
  |                                                                                                                                                                          
  |                        | 1.3.0 & Before  |   32 MB        | Default Setting             |         No        |  N/A                         
  |     A0 / B0                                                                                                                                                           
  |                        | 1.3.0 & Before  |   64 MB        | programming address  |         No        |  N/A                          
  |                                                                          from 0x2000000           |                                                        
  |---------------------------------------------------------------------------------------------------------------------------------------------------
  |                        | 1.4.0 & later     |   32 MB        | Default Setting             |         No        |  N/A                          
  |     A0 / B0                                                                                                                                                        
  |                        | 1.4.0 & later     |   64 MB        | programming address  |         No        |  1.System will random hang during POST
  |                                                                       | from 0x2000000            |         No        |  2.BIOS setup menu value can't chamge  
  |----------------------------------------------------------------------------------------------------------------------------------------------------
  |                        | 1.3.0 & Before  |   32 MB        | Default Setting             |         No        |  System can't boot                    
  |     C0                                                                                                                                                           
  |                        | 1.3.0 & Before  |   64 MB        |  Default Setting            |         No        |   System can't boot                       
  | ------------------------------------------------------------------------------------------------------------------------------------------------------- 
  |                        | 1.4.0 & later     |   32 MB        | Default Setting             |         Yes       |  N/A                         
  |     C0                                                                                                                                                           
  |                        | 1.4.0 & later     |   64 MB        |  Default Setting            |        Yes        |  N/A                          
  | -------------------------------------------------------------------------------------------------------------------------------------------------------                                          
------------
Changes:
------------
1.Set GPIO-115 TO Low when EoP (#485)
2.Support CPM update
3.CPM sign BIOS modify (#483)
4.Modift Setup menu (#475, 476, 477)
5.Fix Build Error whenenable debug mode. (#472)
6.Enable PFR Function

*************************************************************************************
*Version:      00.01.05
*System:       JER15 / JER25 
*              
*Release Date: 05/07/2024
*File Name:    JER25_BIOS_Turin_000105bin
**************************************************************************************
Integrated module collateral:
 AMI CodeBase:
   Turin:0ACST_PI0.0.8.0 (PI 0.0.8.0 / PSP 00.3D.00.52 / SMU 00.5E.4F.00 / U Code (A0 0x0B000048/B0 0x0B001014/C0 0x0B002006 /Dense A0 0xB100008)

---------------
Important Note:
---------------
  1.According AMD Doc#58401 Week-5, Update on 64MB SPI chip usage , It limited the BIOS 
    image update method . Please refer BIOS update SOP when boot with Turin ES1/2 CPU.
  2.Installing Windows Server 2019, 2022, or Windows 10, Windows 11, fails with a blue screen of death (BSOD) error and 
    the message "MULTIPROCESSOR CONFIGURATION NOT SUPPORTED" when installing on the listed AMD-based ThinkSystem platforms 
    that have 64+ cores per CPU package. 
   Workaround:
    1. Reduce the CPU core count in UEFI setting System Information -> Processors -> Number of Enabled CPU Cores Per" to 64C before OS installation.
    2. Install Microsoft Windows Server.
    3. Download and apply the latest Windows Monthly Update from Microsoft's website:
    For Win2022:
       https://support.microsoft.com/en-us/topic/windows-server-2022-update-history-e1caa597-00c5-4ab9-9f3e-8212fe80b2ee
    For Win2019:
       https://support.microsoft.com/en-us/topic/windows-10-and-windows-server-2019-update-history-725fc2e1-4443-6831-a5ca-51ff5cbcb059.
  3. After the update installation is completed, reboot the system and re-enable all CPU cores. The OS should then function as expected.
  4. For Windows client OS (Windows 10 or Windows 11), the recommendation is to download and install 22H2 of Windows 11 to support this type of high core count CPUs.
  5. PCIe Root Bridge has exchange from PI 0.0.8.0 . Therefor the Bus number assign has change , (Before: G3=0x20 , P3=0x60 . After: G3=0x60 , P3=0x20)
  6.Enable PFR function , but request PC (C0 stepping) CPU to support it 
-------------
Known Issues:
-------------
   1.BIOS 0.1.4 can't save setup menu change when use 64 MB Rom part , Suggest change to 32 MB Rom part. 
   2.Rear USB Prt will random fail with BIOS 0.1.4
   3.System will random hang when use 64 MB Rom part , Suggest change to 32 MB Rom part.  

------------
Changes:
------------
1.Reomve Performance setup menu due to it cause system continue reset. (#476,#477)
2.Create item to enable hide setup iten. (#475)
3.Fix compiler build error when debug mode enable.
4.NVMe Hot-Plug Funciotn implement (#448)	
5.BIOS Setup menu adjusting (#449,450,451.452,459,461)	
6.Fix [15669_1] [JER15/25] SMBIOS type 9 information is not match with BIOS spec (#453)
7.Fix [JER15/25][DF15886] SystemInventory porting cpu info (#456)
8.Fix [JER15/25][DF15885] SystemInventory porting dimm info (#457, 458)
9.Fix [DF15748_1] [JER15/25][EVT] SMBIOS type 8 information is not match with BIOS spec. (#460)



*************************************************************************************
*Version:      00.01.04
*System:       JER15 / JER25 
*              
*Release Date: 04/12/2024
*File Name:    JER25_BIOS_Turin_000104bin
**************************************************************************************
Integrated module collateral:
 AMI CodeBase:
   Turin:0ACST_PI0.0.8.0 (PI 0.0.8.0 / PSP 00.3D.00.52 / SMU 00.5E.4F.00 / U Code (A0 0x0B000048/B0 0x0B001014/C0 0x0B002006 /Dense A0 0xB100008)

---------------
Important Note:
---------------
  1.According AMD Doc#58401 Week-5, Update on 64MB SPI chip usage , It limited the BIOS 
    image update method . Please refer BIOS update SOP when boot with Turin ES1/2 CPU.
  2.Installing Windows Server 2019, 2022, or Windows 10, Windows 11, fails with a blue screen of death (BSOD) error and 
    the message "MULTIPROCESSOR CONFIGURATION NOT SUPPORTED" when installing on the listed AMD-based ThinkSystem platforms 
    that have 64+ cores per CPU package. 
   Workaround:
    1. Reduce the CPU core count in UEFI setting System Information -> Processors -> Number of Enabled CPU Cores Per" to 64C before OS installation.
    2. Install Microsoft Windows Server.
    3. Download and apply the latest Windows Monthly Update from Microsoft's website:
    For Win2022:
       https://support.microsoft.com/en-us/topic/windows-server-2022-update-history-e1caa597-00c5-4ab9-9f3e-8212fe80b2ee
    For Win2019:
       https://support.microsoft.com/en-us/topic/windows-10-and-windows-server-2019-update-history-725fc2e1-4443-6831-a5ca-51ff5cbcb059.
  3. After the update installation is completed, reboot the system and re-enable all CPU cores. The OS should then function as expected.
  4. For Windows client OS (Windows 10 or Windows 11), the recommendation is to download and install 22H2 of Windows 11 to support this type of high core count CPUs.
  5. PCIe Root Bridge has exchange from PI 0.0.8.0 . Therefor the Bus number assign has change , (Before: G3=0x20 , P3=0x60 . After: G3=0x60 , P3=0x20)
-------------
Known Issues:
-------------
   1.Hot-plug funciotn not ready.

------------
Changes:
------------
   1. Fix  [JER15/25] PCIe physical slot number update rule.
   2. Fix  [15725/15726] [JER15/25] Add debug log for USB over current warning function analysis
   3. Implement [JER15/JER25] Set GPIO-115 to high when BIOS end of PORT
   4. Fix [440][JER15/25][EVT] SMBIOS type 8 information is not match with BIOS spec.
   5. Fix [JER15/25] DF15665 SystemInventory porting
   6. [15669] [JER15/25] SMBIOS type 9 information is not match with BIOS spec
   7. Fix [15801] [JER15/25][EVT] SMBIOS_Type 41 Onboard Device Extended information is incorrect
   8. Update AMD PI to 0.8.1 from AMD PI-0.7.4

**************************************************************************************
*Version:      00.01.03
*System:       JER15 / JER25 
*              
*Release Date: 03/22/2024
*File Name:    JER25_BIOS_Turin_000103bin
**************************************************************************************
Integrated module collateral:
 AMI CodeBase:
   Turin:0ACST_PI0.0.7.4_010 (PI 7.4 / PSP 00.3D.00.4C / SMU 00.5E.44.00 / U Code (A0 0x0B00003C/B0 0x0B001001/Dense A0 0xB100008)

---------------
Important Note:
---------------
  1.According AMD Doc#58401 Week-5, Update on 64MB SPI chip usage , It limited the BIOS 
    image update method . Please refer BIOS update SOP when boot with Turin ES1/2 CPU.
  2.Installing Windows Server 2019, 2022, or Windows 10, Windows 11, fails with a blue screen of death (BSOD) error and 
    the message "MULTIPROCESSOR CONFIGURATION NOT SUPPORTED" when installing on the listed AMD-based ThinkSystem platforms 
    that have 64+ cores per CPU package. 
   Workaround:
    1. Reduce the CPU core count in UEFI setting System Information -> Processors -> Number of Enabled CPU Cores Per" to 64C before OS installation.
    2. Install Microsoft Windows Server.
    3. Download and apply the latest Windows Monthly Update from Microsoft's website:
    For Win2022:
       https://support.microsoft.com/en-us/topic/windows-server-2022-update-history-e1caa597-00c5-4ab9-9f3e-8212fe80b2ee
    For Win2019:
       https://support.microsoft.com/en-us/topic/windows-10-and-windows-server-2019-update-history-725fc2e1-4443-6831-a5ca-51ff5cbcb059.
    4. After the update installation is completed, reboot the system and re-enable all CPU cores. The OS should then function as expected.
    5. For Windows client OS (Windows 10 or Windows 11), the recommendation is to download and install 22H2 of Windows 11 to support this type of high core count CPUs.
-------------
Known Issues:
-------------
   1.Hot-plug funciotn not ready.
   2.Pcie Slot number asignment not incorrect , and cause some error . 
   3.System inventory function not ready.
   4.There are 2 yellow bang devices in Windows device manager (AMD I2C Controller)

------------
Changes:
------------
   1.[15491] -Issue Fix=> Add channel ID into information String for SMBIOS Type-17 
   2.[15575] -Issue Fix=> Modify Lane reverse related setting.
   3.[15581] -Issue Fix=> Change Aptio HII Style
   4.[15725] -Issue Fix=> Fix incorrect setting for USB controller B/D/F
   5.[15726] -Issue FIX=> Fix incorrect setting for USB controller B/D/F
   6.Modify CPM Build key & IP Address.



**************************************************************************************
*Version:      00.01.02
*System:       JER15 / JER25 
*              
*Release Date: 03/08/2024
*File Name:    JER25_BIOS_Turin_000102.bin
**************************************************************************************
Integrated module collateral:
 AMI CodeBase:
   Turin:0ACST_PI0.0.7.4_010 (PI 7.4 / PSP 00.3D.00.4C / SMU 00.5E.44.00 / U Code (A0 0x0B00003C/B0 0x0B001001/Dense A0 0xB100008)

---------------
Important Note:
---------------
  1.According AMD Doc#58401 Week-5, Update on 64MB SPI chip usage , It limited the BIOS 
    image update method . Please refer BIOS update SOP when boot with Turin ES1/2 CPU.
  2.Installing Windows Server 2019, 2022, or Windows 10, Windows 11, fails with a blue screen of death (BSOD) error and 
    the message "MULTIPROCESSOR CONFIGURATION NOT SUPPORTED" when installing on the listed AMD-based ThinkSystem platforms 
    that have 64+ cores per CPU package. 
   Workaround:
    1. Reduce the CPU core count in UEFI setting System Information -> Processors -> Number of Enabled CPU Cores Per" to 64C before OS installation.
    2. Install Microsoft Windows Server.
    3. Download and apply the latest Windows Monthly Update from Microsoft's website:
    For Win2022:
       https://support.microsoft.com/en-us/topic/windows-server-2022-update-history-e1caa597-00c5-4ab9-9f3e-8212fe80b2ee
    For Win2019:
       https://support.microsoft.com/en-us/topic/windows-10-and-windows-server-2019-update-history-725fc2e1-4443-6831-a5ca-51ff5cbcb059.
    4. After the update installation is completed, reboot the system and re-enable all CPU cores. The OS should then function as expected.
    5. For Windows client OS (Windows 10 or Windows 11), the recommendation is to download and install 22H2 of Windows 11 to support this type of high core count CPUs.
-------------
Known Issues:
-------------
   1.Hot-plug funciotn not ready.
   2.Pcie Slot number asignment not incorrect , and cause some error . 
   3.System inventory function not ready.
   4.NVMe sequency not meet the production spec. 
   5.There are 2 yellow bang devices in Windows device manager (AMD I2C Controller)

------------
Changes:
------------
   1.Update Agesa PI from 0.7.3 to 0.7.4 .
   2.Temp remove SMBIOS type-41 update to avoid Dmidecode fail under linux.  
   3.Add message support for CMOS fail .
   4.Modify GPIO-264/265 pin as USB_OC funciton.



**************************************************************************************
*Version:      00.01.01
*System:       JER15 / JER25 
*              
*Release Date: 02/26/2024
*File Name:    JER25_BIOS_Turin_000101.bin
**************************************************************************************
Integrated module collateral:
 AMI CodeBase:
   Turin:0ACST_PI0.0.7.3_009 (PI 7.3 / PSP 00.3D.00.48 / SMU 00.5E.40.00 / U Code (A0 0x0B00003C/B0 0x0B001001/Dense A0 0xB100006)

---------------
Important Note:
---------------
  1.According AMD Doc#58401 Week-5, Update on 64MB SPI chip usage , It limited the BIOS 
    image update method . Please refer BIOS update SOP when boot with Turin ES1/2 CPU.
  2.Installing Windows Server 2019, 2022, or Windows 10, Windows 11, fails with a blue screen of death (BSOD) error and 
    the message "MULTIPROCESSOR CONFIGURATION NOT SUPPORTED" when installing on the listed AMD-based ThinkSystem platforms 
    that have 64+ cores per CPU package. 
   Workaround:
    1. Reduce the CPU core count in UEFI setting System Information -> Processors -> Number of Enabled CPU Cores Per" to 64C before OS installation.
    2. Install Microsoft Windows Server.
    3. Download and apply the latest Windows Monthly Update from Microsoft's website:
    For Win2022:
       https://support.microsoft.com/en-us/topic/windows-server-2022-update-history-e1caa597-00c5-4ab9-9f3e-8212fe80b2ee
    For Win2019:
       https://support.microsoft.com/en-us/topic/windows-10-and-windows-server-2019-update-history-725fc2e1-4443-6831-a5ca-51ff5cbcb059.
    4. After the update installation is completed, reboot the system and re-enable all CPU cores. The OS should then function as expected.
    5. For Windows client OS (Windows 10 or Windows 11), the recommendation is to download and install 22H2 of Windows 11 to support this type of high core count CPUs.
-------------
Known Issues:
-------------
   1.Hot-plug funciotn not ready.
   2.System will reset if install non-GPU card in GPU Reier-2.
   3.SL-3/SL-4 will cause system reset when installaiton NVMe or other PCIe card. 

------------
Changes:
------------
   1.Implement AC Recovery Function .
   2.Implement Early Video Function .
   2.Fixed #155510 [JER25][EVT] SKU3_Some NVME HDD lost in Windows 2022 built in disk management tool.


**************************************************************************************
*Version:      0.0.1
*System:       JER15 / JER25 
*              
*Release Date: 11/16/2023
*File Name:    JER25_BIOS_Genoa_000001.bin / JER25_BIOS_Turin_000001.bin
**************************************************************************************
Integrated module collateral:
 AMI CodeBase:
   Genoa:0ACQT022 (PI 1.0.0.9 / PSP 00.29.00.93 / SMU 04.71.116.0 / U Code (B0 0x0A101020/B1 0x0A10113E/B2 0x0A10123E)
   Turin:0ACST_PI0.0.7.1_007 (PI 7.1 / PSP 00.3D.00.41 / SMU 00.5E.2E.00 / U Code (A0 0x0B000024/B0 0x0B001001)

---------------
Important Note:
---------------
  Fisrt Release
-------------
KNOWN ISSUES:
-------------
   N/A 
--------
CHANGES:
--------
   N/A



**************************************************************************************
*Version:      00.01.00
*System:       JER15 / JER25 
*              
*Release Date: 02/07/2024
*File Name:    JER25_BIOS_Turin_000001.bin
**************************************************************************************
Integrated module collateral:
 AMI CodeBase:
   Turin:0ACST_PI0.0.7.2_008 (PI 7.2 / PSP 00.3D.00.45 / SMU 00.5E.35.00 / U Code (A0 0x0B000032/B0 0x0B001001/Dense A0 0xB100006)

---------------
Important Note:
---------------
  1.According AMD Doc#58401 Week-5, Update on 64MB SPI chip usage , It limited the BIOS 
    image update method . Please refer BIOS update SOP when boot with Turin ES1/2 CPU.
  2.Installing Windows Server 2019, 2022, or Windows 10, Windows 11, fails with a blue screen of death (BSOD) error and 
    the message "MULTIPROCESSOR CONFIGURATION NOT SUPPORTED" when installing on the listed AMD-based ThinkSystem platforms 
    that have 64+ cores per CPU package. 
   Workaround:
    1. Reduce the CPU core count in UEFI setting System Information -> Processors -> Number of Enabled CPU Cores Per" to 64C before OS installation.
    2. Install Microsoft Windows Server.
    3. Download and apply the latest Windows Monthly Update from Microsoft's website:
    For Win2022:
       https://support.microsoft.com/en-us/topic/windows-server-2022-update-history-e1caa597-00c5-4ab9-9f3e-8212fe80b2ee
    For Win2019:
       https://support.microsoft.com/en-us/topic/windows-10-and-windows-server-2019-update-history-725fc2e1-4443-6831-a5ca-51ff5cbcb059.
    4. After the update installation is completed, reboot the system and re-enable all CPU cores. The OS should then function as expected.
    5. For Windows client OS (Windows 10 or Windows 11), the recommendation is to download and install 22H2 of Windows 11 to support this type of high core count CPUs.
-------------
Known Issues:
-------------
   1.Early Video  not ready.
   2.Hot-plug funciotn not ready.
------------
Changes:
------------
   1.Implement SMbios base on board design.
   2.Implement BP & Riser bifurcation



**************************************************************************************
*Version:      0.0.1
*System:       JER15 / JER25 
*              
*Release Date: 11/16/2023
*File Name:    JER25_BIOS_Genoa_000001.bin / JER25_BIOS_Turin_000001.bin
**************************************************************************************
Integrated module collateral:
 AMI CodeBase:
   Genoa:0ACQT022 (PI 1.0.0.9 / PSP 00.29.00.93 / SMU 04.71.116.0 / U Code (B0 0x0A101020/B1 0x0A10113E/B2 0x0A10123E)
   Turin:0ACST_PI0.0.7.1_007 (PI 7.1 / PSP 00.3D.00.41 / SMU 00.5E.2E.00 / U Code (A0 0x0B000024/B0 0x0B001001)

---------------
Important Note:
---------------
  Fisrt Release
-------------
KNOWN ISSUES:
-------------
   N/A 
--------
CHANGES:
--------
   N/A