The BIOS support the boot block to re-flash the main BIOS image when the BIOS is be 
corrupted and cannot boot to the EFI Shell or operating system to perform a 
standard update. User can jump the recovery jumper to process recovery function. 
 
Step by step :   
1. Copy AMIB.ROM to USB key. 
2. Power off the server and jump the recovery jumper to PIN 2-3 
3. Insert the USB key to the server. 
4. Power on the server and wait system into recovery mode in setup menu. 
5. Select ¡§Proceed with flash update¡¨ and Enter to start flash update. 